### 1.0Shell Service Commands

Shell Service commands are generated from an XML format description of the command tree syntax. It can include localized command help, function calls, and diagnostic tests.

- system
- test
- auth
- show
- upload
- configure
- clear

#### Table 1.1 system Shell Commands

Command | Parameter(s) | Description
--- | --- | ---
system clearcorefiles | clearcorefiles | Remove core generated.
system checkcorefiles | checkcorefiles | Check for core files generated.
system clearcalls | clearcalls | Clear recent calls list.
system reboot | reboot | Reboot the device.
system factoryReset | factoryReset | Reset device to factory default settings.
system rmcalibration | rmcalibration | Remove touchscreen calibration data.
system ping | Ip address of test host | Test reachability of network host.
system ldapsearch | Search entry. | Search for entries in LDAP and local directory.
system traceroute | Ip address of host | Trace route to network host.
system nslookup | Ip address of host | Fetch domain name or IP address from DNS
system provision | provision | Restart provisioning
system deactivateBTService | deactivateBTService | Deactivate the BT Service.
system lldp | lldp | Show LLDP neighbors
system messages | Dump number of lines of syslog messages | Dump syslog messages
system netstat | netstat | Display all network sockets
system eapol | eapol | Display 802.1X authentication status
system bluetooth_svc discover_devices | discover_devices | Scan for devices sending provisioning info
system bluetooth_svc pair | pair | Remote address to pair
system bluetooth_svc gettime | gettime | Get time from paired device
system bluetooth_svc demo | demo | Start/Stop Demo application
system poweruser key | key | Power user key commands
system poweruser packetcapture | packetcapture | Packet capture
system poweruser pds | pds | Power user custom PDS commands
system poweruser appautomation | appautomation | App automation commands

#### Table 1.2 test Shell Commands

Command | Parameter(s) | Description
--- | --- | ---
test audio tones | tones | play tones
test audio tonegen_start | tonegen_start | start tone generator
test audio tonegen_stop | tonegen_stop | stop tone generator
test audio ringer | ringer | play device ringtone
test audio mic | mic | start mic capture
test led red | red |
test led blue | blue |
test led green | green |
test brightness | valid range [0 - 100] | change LCD brightness
test keypadtest | timeout in seconds | Test keypad.

#### Table 1.3 auth Shell Commands

Command | Parameter(s) | Description
--- | --- | ---
auth status | status | Shows authentication service status
auth expireAll | expireAll | Request to expire all active sessions

#### Table 1.4 show Shell Commands

Command | Parameter(s) | Description
--- | --- | ---
show version | version | Shows version
show memory | memory | Display memory usage information.
show cpuload | Display CPU usage informatino of PID. | Display CPU usage information.
show network | network | Display network information.
show date | date | Display date.
show call | call | Display information about call state.
show uptime | uptime | Display information about System uptime.
show disk | disk | Display information about disk state.
show callserver | callserver | Check for call server registration.
show sysload | sysload | Show all system load information.
show dspstate | dspstate | Show DSP state.
show configuration all | all | Show all config params
show configuration running | running | Shows modified configuration
show configuration Features.OperationMode | Features.OperationMode | Device operational mode
show configuration Features.RecentCallsEnabled | Features.RecentCallsEnabled | Flag to determine whether to enable the recent calls feature
show configuration Features.UserFeedback.Enabled | Features.UserFeedback.Enabled | Flag to determine whether to show the call quality feedback dialog at the end of a call
show configuration Features.UserFeedback.Hotline | Features.UserFeedback.Hotline | User feedback hotline number
show configuration Features.PersonalMode.Enabled | Features.PersonalMode.Enabled | By enabling this feature, the phone's owner can save his or her chairperson or host passcode to easily start meetings
show configuration Features.PersonalMode.SecuredAccessEnabled | Features.PersonalMode.SecuredAccessEnabled | Personal PIN authentication required. Only applicable when personal mode is enabled.
show configuration Preferences.DndEnabled | Preferences.DndEnabled | Flag to determine whether to enable the Do Not Disturb feature
show configuration Preferences.AutoAnswerEnabled | Preferences.AutoAnswerEnabled | Flag to determine whether to enable the Auto-Answer feature
show configuration Preferences.ForwardAllNumber | Preferences.ForwardAllNumber | Phone number to which all calls are forwarded
show configuration Preferences.ForwardBusyNumber | Preferences.ForwardBusyNumber | Phone number to which a call is forwarded when the user is busy
show configuration Preferences.ForwardNoAnswerNumber | Preferences.ForwardNoAnswerNumber | Phone number to which a call is forwarded when the user does not answer the call
show configuration Preferences.SpeechVolume | Preferences.SpeechVolume | Speech volume when the Dolby Conference Phone is on a call
show configuration Preferences.RingerVolume | Preferences.RingerVolume | Ringer volume
show configuration Preferences.BrightnessLevel | Preferences.BrightnessLevel | Brightness level of backlight
show configuration Preferences.SystemNotificationSounds | Preferences.SystemNotificationSounds | Turn on or off the system notification sounds
show configuration Preferences.ShowSystemWarning | Preferences.ShowSystemWarning | Show system warning on the phone
show configuration Preferences.Localization.Timezone | Preferences.Localization.Timezone | Time zone where the device is located
show configuration Preferences.Localization.TimeFormat | Preferences.Localization.TimeFormat | Time Format
show configuration Preferences.Localization.DateFormat | Preferences.Localization.DateFormat | Date Format
show configuration Preferences.Localization.Language | Preferences.Localization.Language | Language preference for the embedded UI
show configuration Network.DHCP | Network.DHCP | Flag to determine whether to enable automatic network configuration using DHCP. If true, the phone will request an IP address from the DHCP server. If set to false, the user must manually configure the IP address
show configuration Network.IpAddress | Network.IpAddress | IP address of the phone. Note: Enabled only when Network.DHCP is set to false.
show configuration Network.Subnet | Network.Subnet | Subnet mask of the network interface. Note: Enabled only when Network.DHCP is set to false.
show configuration Network.DefaultGateway | Network.DefaultGateway | Default gateway for IP Routing. Note: Enabled only when Network.DHCP is set to false.
show configuration Network.HostName | Network.HostName | Host name of device
show configuration Network.ManualDNS | Network.ManualDNS | Override DHCP assigned DNS settings
show configuration Network.DomainName | Network.DomainName | Network domain name
show configuration Network.DNS1 | Network.DNS1 | Primary DNS server IP address. Note: Enabled only when Network.DHCP is set to false.
show configuration Network.DNS2 | Network.DNS2 | Secondary DNS server IP address. Note: Enabled only when Network.DHCP is set to false.
show configuration Network.Ethernet.Speed | Network.Ethernet.Speed | Ethernet speed
show configuration Network.Ethernet.Duplex | Network.Ethernet.Duplex | Ethernet duplex
show configuration Network.Ethernet.RxPackets | Network.Ethernet.RxPackets | Total packets received
show configuration Network.Ethernet.TxPackets | Network.Ethernet.TxPackets | Total packets transmitted
show configuration Network.Eapol.Identity | Network.Eapol.Identity | IEEE 802.1X user identity
show configuration Network.Eapol.Password | Network.Eapol.Password | IEEE 802.1X password
show configuration Network.Eapol.CertificateInfo | Network.Eapol.CertificateInfo |
show configuration Network.Eapol.CertificateAcceptedDigest | Network.Eapol.CertificateAcceptedDigest |
show configuration Network.Dhcp.Server | Network.Dhcp.Server | DHCP server IP address
show configuration Network.Ntp.Server1 | Network.Ntp.Server1 | Primary NTP server IP address
show configuration Network.Ntp.Server2 | Network.Ntp.Server2 | Secondary NTP server IP address
show configuration Network.Vlan.ManualVlanId | Network.Vlan.ManualVlanId | User configured VLAN ID. When DHCP does not provide the VLAN ID, this value is used.
show configuration Network.Vlan.ActiveVlanId | Network.Vlan.ActiveVlanId | VLAN ID in use. When provided over DHCP, this parameter is used.
show configuration Network.QoS.DscpVoice | Network.QoS.DscpVoice | Network layer DSCP priority of voice channels
show configuration Network.QoS.DscpSignaling | Network.QoS.DscpSignaling | Network layer DSCP priority of signaling channels
show configuration Network.QoS.CosVoice | Network.QoS.CosVoice | Link layer priority of voice channels
show configuration Network.QoS.CosSignaling | Network.QoS.CosSignaling | Link layer priority of signaling channels
show configuration Network.Proxy.AutoDiscover | Network.Proxy.AutoDiscover | Enable WPAD - Web Proxy Auto-Discovery Protocol
show configuration Network.Proxy.PacUrl | Network.Proxy.PacUrl | PAC (Proxy Auto Configuration) file URL
show configuration Network.Proxy.UserName | Network.Proxy.UserName | Proxy server login name
show configuration Network.Proxy.Password | Network.Proxy.Password | Proxy server login password
show configuration Network.Proxy.EnableCache | Network.Proxy.EnableCache | Enable PAC Cache
show configuration Network.Services.LLDPEnabled | Network.Services.LLDPEnabled | Enable LLDP
show configuration Network.Services.SSHEnabled | Network.Services.SSHEnabled | Enable SSH server
show configuration Network.Services.WebServerMode | Network.Services.WebServerMode | Enable web server
show configuration Network.Status.LinkState | Network.Status.LinkState | Link layer state
show configuration Network.Status.EapolClientCert | Network.Status.EapolClientCert | IEEE 802.1X client certificate
show configuration Network.Status.Eapol | Network.Status.Eapol | IEEE 802.1X authentication status
show configuration Network.Status.EapolMethod | Network.Status.EapolMethod | IEEE 802.1X authentication method in use
show configuration Network.Status.EapolPhase2Method | Network.Status.EapolPhase2Method | IEEE 802.1X authentication phase 2 method
show configuration Network.Status.SpeedDuplexMatch | Network.Status.SpeedDuplexMatch | LLDP Ethernet port speed/duplex match
show configuration Network.Status.LldpNeighbor | Network.Status.LldpNeighbor | Number of LLDP neighbors
show configuration Network.Status.VoiceVlanStatus | Network.Status.VoiceVlanStatus | Voice VLAN status
show configuration Network.Status.Dhcp | Network.Status.Dhcp | DHCP Status
show configuration Network.Status.NtpDiscovery | Network.Status.NtpDiscovery | NTP servers are set by
show configuration Network.Status.WpadStatus | Network.Status.WpadStatus | Web Proxy Auto-Discovery Status
show configuration Network.Status.PacStatus | Network.Status.PacStatus | Proxy Auto-Config Status
show configuration Network.Status.AddressConflict | Network.Status.AddressConflict | IP address conflict
show configuration Network.Status.GatewayStatus | Network.Status.GatewayStatus | Default gateway status
show configuration Network.Status.DnsStatus | Network.Status.DnsStatus | DNS server status
show configuration Network.Status.HostnameResolvable | Network.Status.HostnameResolvable | Device hostname resolvable on DNS server
show configuration Network.Status.ConfigProgress | Network.Status.ConfigProgress | Network configuration progress
show configuration Network.Status.Pds | Network.Status.Pds | PDS connection status
show configuration Network2.Enabled | Network2.Enabled | Flag to determine whether to enable secondary VLAN
show configuration Network2.IpAddress | Network2.IpAddress | IP address of secondary VLAN
show configuration Network2.Subnet | Network2.Subnet | Subnet mask of secondary VLAN
show configuration Network2.DefaultGateway | Network2.DefaultGateway | Default gateway of secondary VLAN
show configuration Network2.DomainName | Network2.DomainName | Network domain name of secondary VLAN
show configuration Network2.DNS1 | Network2.DNS1 | Primary DNS server IP address
show configuration Network2.DNS2 | Network2.DNS2 | Secondary DNS server IP address
show configuration Network2.Dhcp.Server | Network2.Dhcp.Server | DHCP server IP address of secondary VLAN
show configuration Network2.Vlan.ManualVlanId | Network2.Vlan.ManualVlanId | User configured VLAN ID of secondary VLAN
show configuration Network2.Vlan.Name | Network2.Vlan.Name | Secondary VLAN name
show configuration Network2.Proxy.AutoDiscover | Network2.Proxy.AutoDiscover | Enable WPAD - Web Proxy Auto-Discovery Protocol
show configuration Network2.Proxy.PacUrl | Network2.Proxy.PacUrl | PAC Configuration URL
show configuration Network2.Proxy.UserName | Network2.Proxy.UserName | Proxy server login name
show configuration Network2.Proxy.Password | Network2.Proxy.Password | Proxy server login password
show configuration Network2.Status.SecondaryVlan | Network2.Status.SecondaryVlan | Secondary VLAN status
show configuration Network2.Status.Dhcp | Network2.Status.Dhcp | DHCP Status
show configuration Network2.Status.WpadStatus | Network2.Status.WpadStatus | Web Proxy Auto-Discovery Status
show configuration Network2.Status.PacStatus | Network2.Status.PacStatus | Proxy Auto-Config Status
show configuration Network2.Status.AddressConflict | Network2.Status.AddressConflict | IP address conflict
show configuration Network2.Status.GatewayStatus | Network2.Status.GatewayStatus | Default gateway status
show configuration Network2.Status.DnsStatus | Network2.Status.DnsStatus | DNS server status
show configuration Network2.Status.SharedDns | Network2.Status.SharedDns | Share DNS servers with primary VLAN
show configuration Provisioning.Configuration.Files | Provisioning.Configuration.Files | List of configuration files
show configuration Provisioning.Configuration.ImageFile | Provisioning.Configuration.ImageFile | Dolby Conference Phone software image file URL
show configuration Provisioning.CfgChange.UserAcknowledgementEnabled | Provisioning.CfgChange.UserAcknowledgementEnabled | Flag to determine if user acknowledgement is enabled when a configuration change triggers reboot or software update.
show configuration Provisioning.Server.Static | Provisioning.Server.Static | Flag to determine whether to enable static configuration of the provisioning server address. If true, the provisioning server is configurable through Provisioning.Server.Address. If false, the provisioning server information is discovered using bluetooth, DHCP or DNS SRV record.
show configuration Provisioning.Server.PrivacyBlock | Provisioning.Server.PrivacyBlock | Flag to disable all uploads that can violate customer privacy.
show configuration Provisioning.Server.DiscoveryMethod | Provisioning.Server.DiscoveryMethod | Provisioning discovery method
show configuration Provisioning.Server.DiscoveryState | Provisioning.Server.DiscoveryState | Provision discovery status
show configuration Provisioning.Server.Type | Provisioning.Server.Type | Provisioning server type
show configuration Provisioning.Server.Address | Provisioning.Server.Address | Provisioning server address. Note: Enabled only when Provisioning.Server.Static is set to true.
show configuration Provisioning.Server.Username | Provisioning.Server.Username | Provisioning server login name. For example, for Provisioning.Server.Type=ftp, this is the user name for logging into the FTP server.
show configuration Provisioning.Server.Password | Provisioning.Server.Password | Provisioning server login password. For example, for Provisioning.Server.Type=ftp, this is the password for logging into the FTP server.
show configuration Provisioning.Server.UploadDir | Provisioning.Server.UploadDir | Directory on provisioning server for uploaded files
show configuration Provisioning.Scheduled.Enable | Provisioning.Scheduled.Enable | Flag to determine if scheduled provisioning is enabled
show configuration Provisioning.Scheduled.StartTime | Provisioning.Scheduled.StartTime | Scheduled reprovisioning start time
show configuration Provisioning.Scheduled.Duration | Provisioning.Scheduled.Duration | Scheduled reprovisioning interval duration, reprovisioning will happen randomly within this time frame from the start time
show configuration Provisioning.Update.Error | Provisioning.Update.Error | Error number from last update attempt
show configuration Provisioning.InvalidCertificates.Info | Provisioning.InvalidCertificates.Info |
show configuration Provisioning.InvalidCertificates.AcceptedDigests | Provisioning.InvalidCertificates.AcceptedDigests |
show configuration Provisioning.Software.AppVersion | Provisioning.Software.AppVersion | Dolby Conference Phone software version
show configuration Provisioning.Software.VppVersion | Provisioning.Software.VppVersion | Voice Processing Platform version
show configuration Provisioning.Software.AcmeVersion | Provisioning.Software.AcmeVersion | Tunneling Module Version
show configuration Sip.Account.DisplayName | Sip.Account.DisplayName | SIP user display name
show configuration Sip.Account.UserName | Sip.Account.UserName | Extension Number/Address (also used as SIP user name)
show configuration Sip.Account.DisplayNumber | Sip.Account.DisplayNumber | This is the number that will be displayed on the home screen, if not configured then extension number will be displayed instead.
show configuration Sip.Account.TransportType | Sip.Account.TransportType | Preferred transport to communicate with the IP PBX Server
show configuration Sip.Account.SecureMedia | Sip.Account.SecureMedia | Option to specify if secure media (SRTP/SRTCP) is mandatory or optional, applicable only when TLS transport is active
show configuration Sip.Account.SelfPort | Sip.Account.SelfPort | Bind port used for SIP transport. TLS port will be default to UDP/TCP port + 1
show configuration Sip.Pbx.Domain | Sip.Pbx.Domain | The SIP domain is the domain name of the IP PBX service the device is registering with. It should be configured if the device connects to the IP PBX service through one or more SIP Proxies. Leave blank if the device directly connects to the SIP server without going through a SIP proxy.
show configuration Sip.Pbx.OutboundProxy1 | Sip.Pbx.OutboundProxy1 | Primary call server or outbound proxy address
show configuration Sip.Pbx.OutboundProxy1Port | Sip.Pbx.OutboundProxy1Port | Primary call server/Outbound proxy port
show configuration Sip.Pbx.OutboundProxy2 | Sip.Pbx.OutboundProxy2 | Secondary call server or outbound proxy address
show configuration Sip.Pbx.OutboundProxy2Port | Sip.Pbx.OutboundProxy2Port | Secondary SIP server/Outbound Proxy port
show configuration Sip.Pbx.SipUriScheme | Sip.Pbx.SipUriScheme | SIP URI Scheme. When set to true it's sip, when it's set to false it's sips (Secure SIP)
show configuration Sip.Pbx.OnlyAcceptCallServerEvents | Sip.Pbx.OnlyAcceptCallServerEvents | Defines whether the device will only accept SIP events from the IP PBX server
show configuration Sip.Pbx.RegistrationTimeout | Sip.Pbx.RegistrationTimeout | SIP server registration timeout (seconds)
show configuration Sip.Pbx.Codecs | Sip.Pbx.Codecs | PBX Codec list
show configuration Sip.Pbx.InBandDTMF | Sip.Pbx.InBandDTMF | In-band DTMF
show configuration Sip.Credential.Name | Sip.Credential.Name | User credential name
show configuration Sip.Credential.Password | Sip.Credential.Password | User credential password
show configuration Sip.Credential.Realm | Sip.Credential.Realm | Server realm
show configuration Sip.NAT.KeepAliveTimeout | Sip.NAT.KeepAliveTimeout | The keep-alive interval in seconds. Sets the interval at which phones will send a keep-alive packet to the gateway/NAT device to keep the communication port open so that NAT can continue to function.
show configuration Sip.Vad.SignalAnnexB | Sip.Vad.SignalAnnexB | Flag to specify if G729 Annex B should be signaled.
show configuration Dvms.InactiveTalkerTimeout | Dvms.InactiveTalkerTimeout | In BT MeetMe, this parameter defines the timeout to decide when a recent talker becomes inactive so he or she can be removed from the active speaker view
show configuration Dvms.HostPasscode | Dvms.HostPasscode | Chairperson passcode to quickly start meetings. Only applicable when personal mode is enabled.
show configuration Dvms.Service.Provider | Dvms.Service.Provider | Select a service provider from the list
show configuration Dvms.Service.Type | Dvms.Service.Type | Select the conferencing service provider application type
show configuration Dvms.Service.Logo | Dvms.Service.Logo | Select the Dolby Voice audio conferencing service provider logo, that will be displayed on the home screen of the device.
show configuration Dvms.Service.Name | Dvms.Service.Name | Set the Dolby Voice conferencing service name that will appear on the home screen of the device.
show configuration Dvms.Service.EnableBluetoothAdvertisement | Dvms.Service.EnableBluetoothAdvertisement | Allow/disallow Bluetooth Advertisement on DCP
show configuration Dvms.Location.CountryCode | Dvms.Location.CountryCode | Default country code for dial-out
show configuration Dvms.Server.SIPRegistrationRequired | Dvms.Server.SIPRegistrationRequired | Flag to determine if SIP registration is required with the Dolby Voice Conferencing Server
show configuration Dvms.Server.Address | Dvms.Server.Address | Dolby Voice server IP address or domain
show configuration Dvms.Server.Codec | Dvms.Server.Codec | Defines the codec in the SIP SDP offer when connecting to Dolby Voice Conferencing Service
show configuration Dvms.Server.RegistrationPIN | Dvms.Server.RegistrationPIN | Dolby Voice Registration PIN
show configuration Dvms.Server.LogALine | Dvms.Server.LogALine | Enable/Disable conference service logging
show configuration Dvms.PeerDevice.BluetoothId | Dvms.PeerDevice.BluetoothId | Peer device bluetooth ID
show configuration Dvms.PeerDevice.LastUpdateTime | Dvms.PeerDevice.LastUpdateTime | Peer device last update time (number of seconds elapsed since 00:00 UTC 1 Jan 1970)
show configuration Dvms.PeerDevice.CustomData | Dvms.PeerDevice.CustomData | Peer device custom data
show configuration Dvms.PeerDevice.IpAddress | Dvms.PeerDevice.IpAddress | Peer device IP Address
show configuration Dvms.Proxy.Address | Dvms.Proxy.Address | Dolby Voice Conference Proxy Address
show configuration Dvms.Proxy.Port | Dvms.Proxy.Port | Dolby Voice Conference Proxy Port
show configuration Dvms.Proxy.User | Dvms.Proxy.User | Dolby Voice Conference Proxy User
show configuration Dvms.Proxy.Password | Dvms.Proxy.Password | Dolby Voice Conference Proxy Password
show configuration Dvms.Custom.Parameter1 | Dvms.Custom.Parameter1 | Parameter 1 to store the custom configuration
show configuration Dvms.Custom.Parameter2 | Dvms.Custom.Parameter2 | Parameter 2 to store the custom configuration
show configuration Dvms.Custom.Parameter3 | Dvms.Custom.Parameter3 | Parameter 3 to store the custom configuration
show configuration Dvms.Custom.Parameter4 | Dvms.Custom.Parameter4 | Parameter 4 to store the custom configuration
show configuration Dvms.Custom.SecureParameter1 | Dvms.Custom.SecureParameter1 | Secure parameter 1 to store the custom configuration
show configuration Dvms.Custom.SecureParameter2 | Dvms.Custom.SecureParameter2 | Secure parameter 2 to store the custom configuration
show configuration Dvms.Custom.SecureParameter3 | Dvms.Custom.SecureParameter3 | Secure parameter 3 to store the custom configuration
show configuration Dvms.Custom.SecureParameter4 | Dvms.Custom.SecureParameter4 | Secure parameter 4 to store the custom configuration
show configuration Dvms.DeveloperMode.Enabled | Dvms.DeveloperMode.Enabled | Turn on developer mode for the Dolby Conference Phone Conferencing App
show configuration Dvms.Audio.SpatialCaptureOrigin | Dvms.Audio.SpatialCaptureOrigin | To help with audio/video congruence, this parameter allows the application to specify the spatial capture origin so that the audio and video can be aligned
show configuration Dvms.Audio.RoomSize | Dvms.Audio.RoomSize | Optimize performance for a room of this size
show configuration Directory.Ldap.URIList | Directory.Ldap.URIList | Comma-separated list of LDAP server URIs (ldap://xxx[,ldap://yyy])
show configuration Directory.Ldap.LoginName | Directory.Ldap.LoginName | Name used to login into the LDAP server(s)
show configuration Directory.Ldap.Password | Directory.Ldap.Password | Password used to login into the LDAP server(s)
show configuration Directory.Ldap.SecureConnection | Directory.Ldap.SecureConnection | Flag to determine whether to use a secure connection to the LDAP server
show configuration Directory.Ldap.BaseDN | Directory.Ldap.BaseDN | Base domain name for the search. For example, "dc=dolby,dc=com"
show configuration Directory.Ldap.SearchFilter | Directory.Ldap.SearchFilter | LDAP search filter, where %1 is a placeholder for the search keyword
show configuration Directory.Ldap.SearchScope | Directory.Ldap.SearchScope | Search depth, where 0=base, 1=one level down, and 2=sub-tree
show configuration Directory.Ldap.SearchTimeout | Directory.Ldap.SearchTimeout | Search timeout (seconds)
show configuration Directory.Ldap.SearchLimit | Directory.Ldap.SearchLimit | Maximum number of search results
show configuration Directory.Ldap.AttrFirstName | Directory.Ldap.AttrFirstName | Name of the attribute corresponding to the first name in the LDAP schema
show configuration Directory.Ldap.AttrLastName | Directory.Ldap.AttrLastName | Name of the attribute corresponding to the last name in the LDAP schema
show configuration Directory.Ldap.AttrNumber | Directory.Ldap.AttrNumber | Name of the attribute corresponding to the phone number in the LDAP schema
show configuration Directory.Ldap.AttrUUID | Directory.Ldap.AttrUUID | Name of the attribute corresponding to the unique user ID in the LDAP schema
show configuration Directory.Ldap.AttrMail | Directory.Ldap.AttrMail | Name of the attribute corresponding to the e-mail address in the LDAP schema
show configuration Logging.Upload.Enable | Logging.Upload.Enable | Flag to determine if upload of log files is enabled
show configuration Logging.Upload.Interval | Logging.Upload.Interval | Interval between logs uploads in minutes
show configuration Logging.RemoteSyslog.Enable | Logging.RemoteSyslog.Enable | Turn on or off syslog client on the Dolby Conference Phone, configure syslog server IP address to complete the setup
show configuration Logging.RemoteSyslog.Address | Logging.RemoteSyslog.Address | Syslog server IP address
show configuration Logging.Console.EnableOutput | Logging.Console.EnableOutput | Flag to determine if sending of logging messages to active console(s) is enabled
show configuration Logging.Level.Evs | Logging.Level.Evs | EVS (Event Service) is an internal communication dispatch service that allows software modules to talk to each other. In the log file, the module name is EVS.
show configuration Logging.Level.ACME | Logging.Level.ACME | ACME SDK is a 3rd party library that handles tunneling connection with the conferencing service. In the log file, the module name is ACME.
show configuration Logging.Level.DVTSC | Logging.Level.DVTSC | DVTSC SDK is a Dolby library that handles tunneling connection with the conferencing service. In the log file, the module name is DVTS.
show configuration Logging.Level.Sip | Logging.Level.Sip | SIP Communication module, which handles all telephony and conferencing service session negotiation signaling. In the log file, the module name is SIP.
show configuration Logging.Level.Ccapi | Logging.Level.Ccapi | Conference Control API which handles conferencing service signaling for BT MeetMe, such as roster list, active speaker, device registration, etc. In the log file, the module name is CCAPI.
show configuration Logging.Level.Api | Logging.Level.Api | APS API is an application programming interface that is used by the Embedded UI and Web UI. In the log file, the module name is API.
show configuration Logging.Level.Cfg | Logging.Level.Cfg | Configuration manager which handles the storage, dispatch of the configuration parameters. In the log file, the module name is CFG.
show configuration Logging.Level.Auth | Logging.Level.Auth | Authentication module handles user login from the Web UI as well as the SSH shell. In the log file, the module name is AUTH.
show configuration Logging.Level.Web | Logging.Level.Web | Web FastCGI module handles the device Web UI requests for device control and diagnostics. In the log file, the module name is WEB.
show configuration Logging.Level.Ldp | Logging.Level.Ldp | LDAP (Lightweight Directory Access Protocol) handles the LDAP server search request. In the log file, the module name is LDP.
show configuration Logging.Level.Net | Logging.Level.Net | Network service module handles network configuration such as VLAN, DHCP, LLDP, etc. In the log file the module name is NET.
show configuration Logging.Level.Pvs | Logging.Level.Pvs | Provisioning service module handles device interactions with the Provisioning Server. The Provisioning Server is a centralized file server that helps to bulk configure the devices and collect logs. In the log file, the module name is PVS.
show configuration Logging.Level.Shl | Logging.Level.Shl | Shell service handles the SSH shell. In the log file, the module name is SHL.
show configuration Logging.Level.Upd | Logging.Level.Upd | Update service handles the software upgrade process on the device. In the log file, the module name is UPD.
show configuration Logging.Level.Dev | Logging.Level.Dev | Device Manager handles the device hardware-related tasks. In the log file, the module name is DEV.
show configuration Logging.Level.CallLog | Logging.Level.CallLog | Call Log handles the recent call service, records the calls placed, received and missed on the device. In the log file, the module name is CDR.
show configuration Logging.Level.UI | Logging.Level.UI | Embedded UI User interface module. In the log file, the module name is UI.
show configuration Logging.Level.Security | Logging.Level.Security | Security module handles the certificate management of the device. In the log file, the module name is SEC.
show configuration Logging.Level.Cdsp | Logging.Level.Cdsp | DSP (Digital Signal Processor) handles audio processing. In the log file, the module name is CDSP.
show configuration Logging.Level.BLE | Logging.Level.BLE | Bluetooth module. In the log file, the module name is BLE.
show configuration Logging.Level.DCC | Logging.Level.DCC | DCC (Dolby Conferencing Console) module is responsible for communications with the DCC server. In the log file, the module name is DCC.
show configuration Logging.Audio.Mode | Logging.Audio.Mode | Audio module logging level. Possible options are Disabled, Statistics, Diagnostic)
show configuration Logging.Audio.BufferSize | Logging.Audio.BufferSize | Audio logging buffer size in kB. Possible values range from 4096 to 16384
show configuration Logging.Audio.EchoRefInputEnabled | Logging.Audio.EchoRefInputEnabled | Flag to determine if logging of echo reference input is enabled
show configuration Logging.Audio.EchoRefOutputEnabled | Logging.Audio.EchoRefOutputEnabled | Flag to determine if logging of echo reference output is enabled
show configuration Logging.Audio.JitterInputEnabled | Logging.Audio.JitterInputEnabled | Flag to determine if logging of jitter buffer input is enabled
show configuration Logging.Audio.JitterOutputEnabled | Logging.Audio.JitterOutputEnabled | Flag to determine if logging of jitter buffer output is enabled
show configuration Logging.ReportFreeMemory | Logging.ReportFreeMemory | Add memory usage report to each logging entry of the services application
show configuration Device.SerialNumber | Device.SerialNumber | Device serial number
show configuration Device.SetupCompleted | Device.SetupCompleted | Shows device setup completion status
show configuration Device.ConfigurationErrors | Device.ConfigurationErrors | Shows configuration errors
show configuration Device.BoardRevision | Device.BoardRevision | Hardware Revision ID
show configuration Device.CACerts.Total | Device.CACerts.Total | Total number of CA certificates
show configuration Device.CACerts.NotValidYet | Device.CACerts.NotValidYet | Number of not valid yet CA certificates
show configuration Device.CACerts.Expired | Device.CACerts.Expired | Number of expired CA certificates
show configuration Device.CACerts.ExpireSoon | Device.CACerts.ExpireSoon | Number of expiring soon CA certificates
show configuration Device.CACerts.List | Device.CACerts.List | CA certificates details
show configuration Device.SystemResource.ServicesMemoryUsed | Device.SystemResource.ServicesMemoryUsed | Services Mem Usage
show configuration Device.SystemResource.ServicesVirtualMemoryUsed | Device.SystemResource.ServicesVirtualMemoryUsed | Services Virtual Mem Usage
show configuration Device.SystemResource.GUIMemoryUsed | Device.SystemResource.GUIMemoryUsed | GUI Mem Usage
show configuration Device.SystemResource.GUIVirtualMemoryUsed | Device.SystemResource.GUIVirtualMemoryUsed | GUI Virtual Mem Usage
show configuration Device.SystemResource.OverallMemoryUsed | Device.SystemResource.OverallMemoryUsed | Overall Mem Usage
show configuration Device.SystemResource.DSPCPULoad | Device.SystemResource.DSPCPULoad | DSP CPU Load
show configuration Device.SystemResource.DSPMemoryUsage | Device.SystemResource.DSPMemoryUsage | DSP Mem Usage
show configuration Device.SystemResource.ServicesCPULoad | Device.SystemResource.ServicesCPULoad | Services CPU Load
show configuration Device.SystemResource.OverallCPULoad | Device.SystemResource.OverallCPULoad | Overall System CPU Load
show configuration Device.SystemResource.GUICPULoad | Device.SystemResource.GUICPULoad | GUI CPU Load
show configuration Device.SystemResource.UserDataPartitionAvail | Device.SystemResource.UserDataPartitionAvail | The availabble space (KB) in the user data partition
show configuration Device.SystemResource.SystemUptime | Device.SystemResource.SystemUptime | System Uptime
show configuration Device.SystemResource.SystemBootTime | Device.SystemResource.SystemBootTime | System Boot Time (seconds)
show configuration Device.MacAddress | Device.MacAddress | Device MAC address
show configuration Device.Status.SystemWarning | Device.Status.SystemWarning | Overall system warning status
show configuration Device.Status.Network | Device.Status.Network | Primary VLAN Network Status
show configuration Device.Status.Network2 | Device.Status.Network2 | Secondary VLAN Network Status
show configuration Device.Status.SipRegistered | Device.Status.SipRegistered | SIP Registered Status
show configuration Device.Status.SipRegResponse | Device.Status.SipRegResponse | SIP Registration Response
show configuration Device.Status.ActiveSipRegistrar | Device.Status.ActiveSipRegistrar | Address of the active registrar
show configuration Device.Status.ActiveSipTransport | Device.Status.ActiveSipTransport | Current active SIP transport
show configuration Device.Status.NetworkTime | Device.Status.NetworkTime | Time sychronization with network server
show configuration Device.Status.BTMeetMeRegistered | Device.Status.BTMeetMeRegistered | BT MeetMe Registration Status
show configuration Device.Status.LDAPConnected | Device.Status.LDAPConnected | LDAP Connected Status
show configuration Device.Status.ProvisionSuccessful | Device.Status.ProvisionSuccessful | Provision Successful Status
show configuration Device.Status.SoftwareUpdateSuccessful | Device.Status.SoftwareUpdateSuccessful | Software Update Successful Status
show configuration Device.Status.LogsUpload | Device.Status.LogsUpload | Logs Upload Successful Status
show configuration Device.Status.LoggingImpact | Device.Status.LoggingImpact | Logging Impact On Performance Status
show configuration Device.Status.Reboot | Device.Status.Reboot | Shows device reboot status
show configuration Device.Status.CallInProgress | Device.Status.CallInProgress | Shows call progress status
show configuration Device.Status.CACertificates | Device.Status.CACertificates | Shows imported CA certificate status
show configuration Device.Status.SatMicConnections | Device.Status.SatMicConnections | Shows Satellite Microphone Connection State
show configuration Device.Status.BluetoothModuleInitialized | Device.Status.BluetoothModuleInitialized | Indicates if Bluetooth module initialized successfully
show configuration Device.App.Status | Device.App.Status | Application status
show configuration Device.App.Version | Device.App.Version | Application version
show configuration Device.App.Name | Device.App.Name | Application name
show configuration Device.OOBApp.Address | Device.OOBApp.Address | OOBE Application URL
show configuration Device.AppRecording | Device.AppRecording | Enables the recording of mouse actions from the Applicatiion
show configuration Device.ReportCrashToDolby | Device.ReportCrashToDolby | Enables the reporting of diagnostics information to Dolby error reporting service
show configuration Authentication.Local.Admin | Authentication.Local.Admin | Administrative password
show configuration Authentication.Local.SessionTimeout | Authentication.Local.SessionTimeout | Default authenticated session timeout in seconds. A session is created when a user logs in from Web UI or command line interface
show configuration Authentication.Local.SessionPurgeTime | Authentication.Local.SessionPurgeTime | The expired sessions record will be purged from the internal sessions list after this many seconds
show configuration Authentication.Local.AccessPin | Authentication.Local.AccessPin | Phone access PIN. Only applicable when secured access is enabled.
show configuration Authentication.Local.AutoLockDuration | Authentication.Local.AutoLockDuration | Duration of auto-lock timeout. Only applicable when secured access is enabled for personal mode in the BT MeetMe scenario.
show authStatus | authStatus | Shows authentication service status

#### Table 1.5 upload Shell Commands

Command | Parameter(s) | Description
--- | --- | ---
upload audiolog | audiolog | Upload audio logs.

#### Table 1.6 configure Shell Commands

Command | Parameter(s) | Description
--- | --- | ---
configure Features.OperationMode | Features.OperationMode | Device operational mode
configure Features.RecentCallsEnabled | Features.RecentCallsEnabled | Flag to determine whether to enable the recent calls feature
configure Features.UserFeedback.Enabled | Features.UserFeedback.Enabled | Flag to determine whether to show the call quality feedback dialog at the end of a call
configure Features.UserFeedback.Hotline | Features.UserFeedback.Hotline | User feedback hotline number
configure Features.PersonalMode.Enabled | Features.PersonalMode.Enabled | By enabling this feature, the phone's owner can save his or her chairperson or host passcode to easily start meetings
configure Features.PersonalMode.SecuredAccessEnabled | Features.PersonalMode.SecuredAccessEnabled | Personal PIN authentication required. Only applicable when personal mode is enabled.
configure Preferences.DndEnabled | Preferences.DndEnabled | Flag to determine whether to enable the Do Not Disturb feature
configure Preferences.AutoAnswerEnabled | Preferences.AutoAnswerEnabled | Flag to determine whether to enable the Auto-Answer feature
configure Preferences.ForwardAllNumber | Preferences.ForwardAllNumber | Phone number to which all calls are forwarded
configure Preferences.ForwardBusyNumber | Preferences.ForwardBusyNumber | Phone number to which a call is forwarded when the user is busy
configure Preferences.ForwardNoAnswerNumber | Preferences.ForwardNoAnswerNumber | Phone number to which a call is forwarded when the user does not answer the call
configure Preferences.SpeechVolume | Preferences.SpeechVolume | Speech volume when the Dolby Conference Phone is on a call
configure Preferences.RingerVolume | Preferences.RingerVolume | Ringer volume
configure Preferences.BrightnessLevel | Preferences.BrightnessLevel | Brightness level of backlight
configure Preferences.SystemNotificationSounds | Preferences.SystemNotificationSounds | Turn on or off the system notification sounds
configure Preferences.ShowSystemWarning | Preferences.ShowSystemWarning | Show system warning on the phone
configure Preferences.Localization.Timezone | Preferences.Localization.Timezone | Time zone where the device is located
configure Preferences.Localization.TimeFormat | Preferences.Localization.TimeFormat | Time Format
configure Preferences.Localization.DateFormat | Preferences.Localization.DateFormat | Date Format
configure Preferences.Localization.Language | Preferences.Localization.Language | Language preference for the embedded UI
configure Network.DHCP | Network.DHCP | Flag to determine whether to enable automatic network configuration using DHCP. If true, the phone will request an IP address from the DHCP server. If set to false, the user must manually configure the IP address
configure Network.IpAddress | Network.IpAddress | IP address of the phone. Note: Enabled only when Network.DHCP is set to false.
configure Network.Subnet | Network.Subnet | Subnet mask of the network interface. Note: Enabled only when Network.DHCP is set to false.
configure Network.DefaultGateway | Network.DefaultGateway | Default gateway for IP Routing. Note: Enabled only when Network.DHCP is set to false.
configure Network.ManualDNS | Network.ManualDNS | Override DHCP assigned DNS settings
configure Network.DomainName | Network.DomainName | Network domain name
configure Network.DNS1 | Network.DNS1 | Primary DNS server IP address. Note: Enabled only when Network.DHCP is set to false.
configure Network.DNS2 | Network.DNS2 | Secondary DNS server IP address. Note: Enabled only when Network.DHCP is set to false.
configure Network.Eapol.Identity | Network.Eapol.Identity | IEEE 802.1X user identity
configure Network.Eapol.Password | Network.Eapol.Password | IEEE 802.1X password
configure Network.Eapol.CertificateAcceptedDigest | Network.Eapol.CertificateAcceptedDigest |
configure Network.Ntp.Server1 | Network.Ntp.Server1 | Primary NTP server IP address
configure Network.Ntp.Server2 | Network.Ntp.Server2 | Secondary NTP server IP address
configure Network.Vlan.ManualVlanId | Network.Vlan.ManualVlanId | User configured VLAN ID. When DHCP does not provide the VLAN ID, this value is used.
configure Network.QoS.DscpVoice | Network.QoS.DscpVoice | Network layer DSCP priority of voice channels
configure Network.QoS.DscpSignaling | Network.QoS.DscpSignaling | Network layer DSCP priority of signaling channels
configure Network.QoS.CosVoice | Network.QoS.CosVoice | Link layer priority of voice channels
configure Network.QoS.CosSignaling | Network.QoS.CosSignaling | Link layer priority of signaling channels
configure Network.Proxy.AutoDiscover | Network.Proxy.AutoDiscover | Enable WPAD - Web Proxy Auto-Discovery Protocol
configure Network.Proxy.PacUrl | Network.Proxy.PacUrl | PAC (Proxy Auto Configuration) file URL
configure Network.Proxy.UserName | Network.Proxy.UserName | Proxy server login name
configure Network.Proxy.Password | Network.Proxy.Password | Proxy server login password
configure Network.Proxy.EnableCache | Network.Proxy.EnableCache | Enable PAC Cache
configure Network.Services.LLDPEnabled | Network.Services.LLDPEnabled | Enable LLDP
configure Network.Services.SSHEnabled | Network.Services.SSHEnabled | Enable SSH server
configure Network.Services.WebServerMode | Network.Services.WebServerMode | Enable web server
configure Network2.Enabled | Network2.Enabled | Flag to determine whether to enable secondary VLAN
configure Network2.Vlan.ManualVlanId | Network2.Vlan.ManualVlanId | User configured VLAN ID of secondary VLAN
configure Network2.Proxy.AutoDiscover | Network2.Proxy.AutoDiscover | Enable WPAD - Web Proxy Auto-Discovery Protocol
configure Network2.Proxy.PacUrl | Network2.Proxy.PacUrl | PAC Configuration URL
configure Network2.Proxy.UserName | Network2.Proxy.UserName | Proxy server login name
configure Network2.Proxy.Password | Network2.Proxy.Password | Proxy server login password
configure Provisioning.CfgChange.UserAcknowledgementEnabled | Provisioning.CfgChange.UserAcknowledgementEnabled | Flag to determine if user acknowledgement is enabled when a configuration change triggers reboot or software update.
configure Provisioning.Server.Static | Provisioning.Server.Static | Flag to determine whether to enable static configuration of the provisioning server address. If true, the provisioning server is configurable through Provisioning.Server.Address. If false, the provisioning server information is discovered using bluetooth, DHCP or DNS SRV record.
configure Provisioning.Server.PrivacyBlock | Provisioning.Server.PrivacyBlock | Flag to disable all uploads that can violate customer privacy.
configure Provisioning.Server.DiscoveryMethod | Provisioning.Server.DiscoveryMethod | Provisioning discovery method
configure Provisioning.Server.Type | Provisioning.Server.Type | Provisioning server type
configure Provisioning.Server.Address | Provisioning.Server.Address | Provisioning server address. Note: Enabled only when Provisioning.Server.Static is set to true.
configure Provisioning.Server.Username | Provisioning.Server.Username | Provisioning server login name. For example, for Provisioning.Server.Type=ftp, this is the user name for logging into the FTP server.
configure Provisioning.Server.Password | Provisioning.Server.Password | Provisioning server login password. For example, for Provisioning.Server.Type=ftp, this is the password for logging into the FTP server.
configure Provisioning.Server.UploadDir | Provisioning.Server.UploadDir | Directory on provisioning server for uploaded files
configure Provisioning.Scheduled.Enable | Provisioning.Scheduled.Enable | Flag to determine if scheduled provisioning is enabled
configure Provisioning.Scheduled.StartTime | Provisioning.Scheduled.StartTime | Scheduled reprovisioning start time
configure Provisioning.Scheduled.Duration | Provisioning.Scheduled.Duration | Scheduled reprovisioning interval duration, reprovisioning will happen randomly within this time frame from the start time
configure Provisioning.InvalidCertificates.AcceptedDigests | Provisioning.InvalidCertificates.AcceptedDigests |
configure Sip.Account.DisplayName | Sip.Account.DisplayName | SIP user display name
configure Sip.Account.UserName | Sip.Account.UserName | Extension Number/Address (also used as SIP user name)
configure Sip.Account.DisplayNumber | Sip.Account.DisplayNumber | This is the number that will be displayed on the home screen, if not configured then extension number will be displayed instead.
configure Sip.Account.TransportType | Sip.Account.TransportType | Preferred transport to communicate with the IP PBX Server
configure Sip.Account.SecureMedia | Sip.Account.SecureMedia | Option to specify if secure media (SRTP/SRTCP) is mandatory or optional, applicable only when TLS transport is active
configure Sip.Account.SelfPort | Sip.Account.SelfPort | Bind port used for SIP transport. TLS port will be default to UDP/TCP port + 1
configure Sip.Pbx.Domain | Sip.Pbx.Domain | The SIP domain is the domain name of the IP PBX service the device is registering with. It should be configured if the device connects to the IP PBX service through one or more SIP Proxies. Leave blank if the device directly connects to the SIP server without going through a SIP proxy.
configure Sip.Pbx.OutboundProxy1 | Sip.Pbx.OutboundProxy1 | Primary call server or outbound proxy address
configure Sip.Pbx.OutboundProxy1Port | Sip.Pbx.OutboundProxy1Port | Primary call server/Outbound proxy port
configure Sip.Pbx.OutboundProxy2 | Sip.Pbx.OutboundProxy2 | Secondary call server or outbound proxy address
configure Sip.Pbx.OutboundProxy2Port | Sip.Pbx.OutboundProxy2Port | Secondary SIP server/Outbound Proxy port
configure Sip.Pbx.SipUriScheme | Sip.Pbx.SipUriScheme | SIP URI Scheme. When set to true it's sip, when it's set to false it's sips (Secure SIP)
configure Sip.Pbx.OnlyAcceptCallServerEvents | Sip.Pbx.OnlyAcceptCallServerEvents | Defines whether the device will only accept SIP events from the IP PBX server
configure Sip.Pbx.RegistrationTimeout | Sip.Pbx.RegistrationTimeout | SIP server registration timeout (seconds)
configure Sip.Pbx.Codecs | Sip.Pbx.Codecs | PBX Codec list
configure Sip.Pbx.InBandDTMF | Sip.Pbx.InBandDTMF | In-band DTMF
configure Sip.Credential.Name | Sip.Credential.Name | User credential name
configure Sip.Credential.Password | Sip.Credential.Password | User credential password
configure Sip.Credential.Realm | Sip.Credential.Realm | Server realm
configure Sip.NAT.KeepAliveTimeout | Sip.NAT.KeepAliveTimeout | The keep-alive interval in seconds. Sets the interval at which phones will send a keep-alive packet to the gateway/NAT device to keep the communication port open so that NAT can continue to function.
configure Sip.Vad.SignalAnnexB | Sip.Vad.SignalAnnexB | Flag to specify if G729 Annex B should be signaled.
configure Dvms.InactiveTalkerTimeout | Dvms.InactiveTalkerTimeout | In BT MeetMe, this parameter defines the timeout to decide when a recent talker becomes inactive so he or she can be removed from the active speaker view
configure Dvms.HostPasscode | Dvms.HostPasscode | Chairperson passcode to quickly start meetings. Only applicable when personal mode is enabled.
configure Dvms.Service.Provider | Dvms.Service.Provider | Select a service provider from the list
configure Dvms.Service.Type | Dvms.Service.Type | Select the conferencing service provider application type
configure Dvms.Service.Logo | Dvms.Service.Logo | Select the Dolby Voice audio conferencing service provider logo, that will be displayed on the home screen of the device.
configure Dvms.Service.Name | Dvms.Service.Name | Set the Dolby Voice conferencing service name that will appear on the home screen of the device.
configure Dvms.Service.EnableBluetoothAdvertisement | Dvms.Service.EnableBluetoothAdvertisement | Allow/disallow Bluetooth Advertisement on DCP
configure Dvms.Location.CountryCode | Dvms.Location.CountryCode | Default country code for dial-out
configure Dvms.Server.SIPRegistrationRequired | Dvms.Server.SIPRegistrationRequired | Flag to determine if SIP registration is required with the Dolby Voice Conferencing Server
configure Dvms.Server.Address | Dvms.Server.Address | Dolby Voice server IP address or domain
configure Dvms.Server.Codec | Dvms.Server.Codec | Defines the codec in the SIP SDP offer when connecting to Dolby Voice Conferencing Service
configure Dvms.Server.RegistrationPIN | Dvms.Server.RegistrationPIN | Dolby Voice Registration PIN
configure Dvms.Server.LogALine | Dvms.Server.LogALine | Enable/Disable conference service logging
configure Dvms.PeerDevice.BluetoothId | Dvms.PeerDevice.BluetoothId | Peer device bluetooth ID
configure Dvms.PeerDevice.IpAddress | Dvms.PeerDevice.IpAddress | Peer device IP Address
configure Dvms.Proxy.Address | Dvms.Proxy.Address | Dolby Voice Conference Proxy Address
configure Dvms.Proxy.Port | Dvms.Proxy.Port | Dolby Voice Conference Proxy Port
configure Dvms.Proxy.User | Dvms.Proxy.User | Dolby Voice Conference Proxy User
configure Dvms.Proxy.Password | Dvms.Proxy.Password | Dolby Voice Conference Proxy Password
configure Dvms.Custom.Parameter1 | Dvms.Custom.Parameter1 | Parameter 1 to store the custom configuration
configure Dvms.Custom.Parameter2 | Dvms.Custom.Parameter2 | Parameter 2 to store the custom configuration
configure Dvms.Custom.Parameter3 | Dvms.Custom.Parameter3 | Parameter 3 to store the custom configuration
configure Dvms.Custom.Parameter4 | Dvms.Custom.Parameter4 | Parameter 4 to store the custom configuration
configure Dvms.Custom.SecureParameter1 | Dvms.Custom.SecureParameter1 | Secure parameter 1 to store the custom configuration
configure Dvms.Custom.SecureParameter2 | Dvms.Custom.SecureParameter2 | Secure parameter 2 to store the custom configuration
configure Dvms.Custom.SecureParameter3 | Dvms.Custom.SecureParameter3 | Secure parameter 3 to store the custom configuration
configure Dvms.Custom.SecureParameter4 | Dvms.Custom.SecureParameter4 | Secure parameter 4 to store the custom configuration
configure Dvms.DeveloperMode.Enabled | Dvms.DeveloperMode.Enabled | Turn on developer mode for the Dolby Conference Phone Conferencing App
configure Dvms.Audio.SpatialCaptureOrigin | Dvms.Audio.SpatialCaptureOrigin | To help with audio/video congruence, this parameter allows the application to specify the spatial capture origin so that the audio and video can be aligned
configure Dvms.Audio.RoomSize | Dvms.Audio.RoomSize | Optimize performance for a room of this size
configure Directory.Ldap.URIList | Directory.Ldap.URIList | Comma-separated list of LDAP server URIs (ldap://xxx[,ldap://yyy])
configure Directory.Ldap.LoginName | Directory.Ldap.LoginName | Name used to login into the LDAP server(s)
configure Directory.Ldap.Password | Directory.Ldap.Password | Password used to login into the LDAP server(s)
configure Directory.Ldap.SecureConnection | Directory.Ldap.SecureConnection | Flag to determine whether to use a secure connection to the LDAP server
configure Directory.Ldap.BaseDN | Directory.Ldap.BaseDN | Base domain name for the search. For example, "dc=dolby,dc=com"
configure Directory.Ldap.SearchFilter | Directory.Ldap.SearchFilter | LDAP search filter, where %1 is a placeholder for the search keyword
configure Directory.Ldap.SearchScope | Directory.Ldap.SearchScope | Search depth, where 0=base, 1=one level down, and 2=sub-tree
configure Directory.Ldap.SearchTimeout | Directory.Ldap.SearchTimeout | Search timeout (seconds)
configure Directory.Ldap.SearchLimit | Directory.Ldap.SearchLimit | Maximum number of search results
configure Directory.Ldap.AttrFirstName | Directory.Ldap.AttrFirstName | Name of the attribute corresponding to the first name in the LDAP schema
configure Directory.Ldap.AttrLastName | Directory.Ldap.AttrLastName | Name of the attribute corresponding to the last name in the LDAP schema
configure Directory.Ldap.AttrNumber | Directory.Ldap.AttrNumber | Name of the attribute corresponding to the phone number in the LDAP schema
configure Directory.Ldap.AttrUUID | Directory.Ldap.AttrUUID | Name of the attribute corresponding to the unique user ID in the LDAP schema
configure Directory.Ldap.AttrMail | Directory.Ldap.AttrMail | Name of the attribute corresponding to the e-mail address in the LDAP schema
configure Logging.Upload.Enable | Logging.Upload.Enable | Flag to determine if upload of log files is enabled
configure Logging.Upload.Interval | Logging.Upload.Interval | Interval between logs uploads in minutes
configure Logging.RemoteSyslog.Enable | Logging.RemoteSyslog.Enable | Turn on or off syslog client on the Dolby Conference Phone, configure syslog server IP address to complete the setup
configure Logging.RemoteSyslog.Address | Logging.RemoteSyslog.Address | Syslog server IP address
configure Logging.Console.EnableOutput | Logging.Console.EnableOutput | Flag to determine if sending of logging messages to active console(s) is enabled
configure Logging.Level.Evs | Logging.Level.Evs | EVS (Event Service) is an internal communication dispatch service that allows software modules to talk to each other. In the log file, the module name is EVS.
configure Logging.Level.ACME | Logging.Level.ACME | ACME SDK is a 3rd party library that handles tunneling connection with the conferencing service. In the log file, the module name is ACME.
configure Logging.Level.DVTSC | Logging.Level.DVTSC | DVTSC SDK is a Dolby library that handles tunneling connection with the conferencing service. In the log file, the module name is DVTS.
configure Logging.Level.Sip | Logging.Level.Sip | SIP Communication module, which handles all telephony and conferencing service session negotiation signaling. In the log file, the module name is SIP.
configure Logging.Level.Ccapi | Logging.Level.Ccapi | Conference Control API which handles conferencing service signaling for BT MeetMe, such as roster list, active speaker, device registration, etc. In the log file, the module name is CCAPI.
configure Logging.Level.Api | Logging.Level.Api | APS API is an application programming interface that is used by the Embedded UI and Web UI. In the log file, the module name is API.
configure Logging.Level.Cfg | Logging.Level.Cfg | Configuration manager which handles the storage, dispatch of the configuration parameters. In the log file, the module name is CFG.
configure Logging.Level.Auth | Logging.Level.Auth | Authentication module handles user login from the Web UI as well as the SSH shell. In the log file, the module name is AUTH.
configure Logging.Level.Web | Logging.Level.Web | Web FastCGI module handles the device Web UI requests for device control and diagnostics. In the log file, the module name is WEB.
configure Logging.Level.Ldp | Logging.Level.Ldp | LDAP (Lightweight Directory Access Protocol) handles the LDAP server search request. In the log file, the module name is LDP.
configure Logging.Level.Net | Logging.Level.Net | Network service module handles network configuration such as VLAN, DHCP, LLDP, etc. In the log file the module name is NET.
configure Logging.Level.Pvs | Logging.Level.Pvs | Provisioning service module handles device interactions with the Provisioning Server. The Provisioning Server is a centralized file server that helps to bulk configure the devices and collect logs. In the log file, the module name is PVS.
configure Logging.Level.Shl | Logging.Level.Shl | Shell service handles the SSH shell. In the log file, the module name is SHL.
configure Logging.Level.Upd | Logging.Level.Upd | Update service handles the software upgrade process on the device. In the log file, the module name is UPD.
configure Logging.Level.Dev | Logging.Level.Dev | Device Manager handles the device hardware-related tasks. In the log file, the module name is DEV.
configure Logging.Level.CallLog | Logging.Level.CallLog | Call Log handles the recent call service, records the calls placed, received and missed on the device. In the log file, the module name is CDR.
configure Logging.Level.UI | Logging.Level.UI | Embedded UI User interface module. In the log file, the module name is UI.
configure Logging.Level.Security | Logging.Level.Security | Security module handles the certificate management of the device. In the log file, the module name is SEC.
configure Logging.Level.Cdsp | Logging.Level.Cdsp | DSP (Digital Signal Processor) handles audio processing. In the log file, the module name is CDSP.
configure Logging.Level.BLE | Logging.Level.BLE | Bluetooth module. In the log file, the module name is BLE.
configure Logging.Level.DCC | Logging.Level.DCC | DCC (Dolby Conferencing Console) module is responsible for communications with the DCC server. In the log file, the module name is DCC.
configure Logging.Audio.Mode | Logging.Audio.Mode | Audio module logging level. Possible options are Disabled, Statistics, Diagnostic)
configure Logging.Audio.BufferSize | Logging.Audio.BufferSize | Audio logging buffer size in kB. Possible values range from 4096 to 16384
configure Logging.Audio.EchoRefInputEnabled | Logging.Audio.EchoRefInputEnabled | Flag to determine if logging of echo reference input is enabled
configure Logging.Audio.EchoRefOutputEnabled | Logging.Audio.EchoRefOutputEnabled | Flag to determine if logging of echo reference output is enabled
configure Logging.Audio.JitterInputEnabled | Logging.Audio.JitterInputEnabled | Flag to determine if logging of jitter buffer input is enabled
configure Logging.Audio.JitterOutputEnabled | Logging.Audio.JitterOutputEnabled | Flag to determine if logging of jitter buffer output is enabled
configure Logging.ReportFreeMemory | Logging.ReportFreeMemory | Add memory usage report to each logging entry of the services application
configure Device.SetupCompleted | Device.SetupCompleted | Shows device setup completion status
configure Device.Status.Reboot | Device.Status.Reboot | Shows device reboot status
configure Device.App.Status | Device.App.Status | Application status
configure Device.App.Version | Device.App.Version | Application version
configure Device.App.Name | Device.App.Name | Application name
configure Device.OOBApp.Address | Device.OOBApp.Address | OOBE Application URL
configure Device.AppRecording | Device.AppRecording | Enables the recording of mouse actions from the Applicatiion
configure Device.ReportCrashToDolby | Device.ReportCrashToDolby | Enables the reporting of diagnostics information to Dolby error reporting service
configure Authentication.Local.Admin | Authentication.Local.Admin | Administrative password
configure Authentication.Local.SessionTimeout | Authentication.Local.SessionTimeout | Default authenticated session timeout in seconds. A session is created when a user logs in from Web UI or command line interface
configure Authentication.Local.SessionPurgeTime | Authentication.Local.SessionPurgeTime | The expired sessions record will be purged from the internal sessions list after this many seconds
configure Authentication.Local.AccessPin | Authentication.Local.AccessPin | Phone access PIN. Only applicable when secured access is enabled.
configure Authentication.Local.AutoLockDuration | Authentication.Local.AutoLockDuration | Duration of auto-lock timeout. Only applicable when secured access is enabled for personal mode in the BT MeetMe scenario.

#### Table 1.7 clear Shell Commands

Command | Parameter(s) | Description
--- | --- | ---
clear Features.OperationMode | Features.OperationMode | Device operational mode
clear Features.RecentCallsEnabled | Features.RecentCallsEnabled | Flag to determine whether to enable the recent calls feature
clear Features.UserFeedback.Enabled | Features.UserFeedback.Enabled | Flag to determine whether to show the call quality feedback dialog at the end of a call
clear Features.UserFeedback.Hotline | Features.UserFeedback.Hotline | User feedback hotline number
clear Features.PersonalMode.Enabled | Features.PersonalMode.Enabled | By enabling this feature, the phone's owner can save his or her chairperson or host passcode to easily start meetings
clear Features.PersonalMode.SecuredAccessEnabled | Features.PersonalMode.SecuredAccessEnabled | Personal PIN authentication required. Only applicable when personal mode is enabled.
clear Preferences.DndEnabled | Preferences.DndEnabled | Flag to determine whether to enable the Do Not Disturb feature
clear Preferences.AutoAnswerEnabled | Preferences.AutoAnswerEnabled | Flag to determine whether to enable the Auto-Answer feature
clear Preferences.ForwardAllNumber | Preferences.ForwardAllNumber | Phone number to which all calls are forwarded
clear Preferences.ForwardBusyNumber | Preferences.ForwardBusyNumber | Phone number to which a call is forwarded when the user is busy
clear Preferences.ForwardNoAnswerNumber | Preferences.ForwardNoAnswerNumber | Phone number to which a call is forwarded when the user does not answer the call
clear Preferences.SpeechVolume | Preferences.SpeechVolume | Speech volume when the Dolby Conference Phone is on a call
clear Preferences.RingerVolume | Preferences.RingerVolume | Ringer volume
clear Preferences.BrightnessLevel | Preferences.BrightnessLevel | Brightness level of backlight
clear Preferences.SystemNotificationSounds | Preferences.SystemNotificationSounds | Turn on or off the system notification sounds
clear Preferences.ShowSystemWarning | Preferences.ShowSystemWarning | Show system warning on the phone
clear Preferences.Localization.Timezone | Preferences.Localization.Timezone | Time zone where the device is located
clear Preferences.Localization.TimeFormat | Preferences.Localization.TimeFormat | Time Format
clear Preferences.Localization.DateFormat | Preferences.Localization.DateFormat | Date Format
clear Preferences.Localization.Language | Preferences.Localization.Language | Language preference for the embedded UI
clear Network.DHCP | Network.DHCP | Flag to determine whether to enable automatic network configuration using DHCP. If true, the phone will request an IP address from the DHCP server. If set to false, the user must manually configure the IP address
clear Network.IpAddress | Network.IpAddress | IP address of the phone. Note: Enabled only when Network.DHCP is set to false.
clear Network.Subnet | Network.Subnet | Subnet mask of the network interface. Note: Enabled only when Network.DHCP is set to false.
clear Network.DefaultGateway | Network.DefaultGateway | Default gateway for IP Routing. Note: Enabled only when Network.DHCP is set to false.
clear Network.ManualDNS | Network.ManualDNS | Override DHCP assigned DNS settings
clear Network.DomainName | Network.DomainName | Network domain name
clear Network.DNS1 | Network.DNS1 | Primary DNS server IP address. Note: Enabled only when Network.DHCP is set to false.
clear Network.DNS2 | Network.DNS2 | Secondary DNS server IP address. Note: Enabled only when Network.DHCP is set to false.
clear Network.Eapol.Identity | Network.Eapol.Identity | IEEE 802.1X user identity
clear Network.Eapol.Password | Network.Eapol.Password | IEEE 802.1X password
clear Network.Eapol.CertificateAcceptedDigest | Network.Eapol.CertificateAcceptedDigest |
clear Network.Ntp.Server1 | Network.Ntp.Server1 | Primary NTP server IP address
clear Network.Ntp.Server2 | Network.Ntp.Server2 | Secondary NTP server IP address
clear Network.Vlan.ManualVlanId | Network.Vlan.ManualVlanId | User configured VLAN ID. When DHCP does not provide the VLAN ID, this value is used.
clear Network.QoS.DscpVoice | Network.QoS.DscpVoice | Network layer DSCP priority of voice channels
clear Network.QoS.DscpSignaling | Network.QoS.DscpSignaling | Network layer DSCP priority of signaling channels
clear Network.QoS.CosVoice | Network.QoS.CosVoice | Link layer priority of voice channels
clear Network.QoS.CosSignaling | Network.QoS.CosSignaling | Link layer priority of signaling channels
clear Network.Proxy.AutoDiscover | Network.Proxy.AutoDiscover | Enable WPAD - Web Proxy Auto-Discovery Protocol
clear Network.Proxy.PacUrl | Network.Proxy.PacUrl | PAC (Proxy Auto Configuration) file URL
clear Network.Proxy.UserName | Network.Proxy.UserName | Proxy server login name
clear Network.Proxy.Password | Network.Proxy.Password | Proxy server login password
clear Network.Proxy.EnableCache | Network.Proxy.EnableCache | Enable PAC Cache
clear Network.Services.LLDPEnabled | Network.Services.LLDPEnabled | Enable LLDP
clear Network.Services.SSHEnabled | Network.Services.SSHEnabled | Enable SSH server
clear Network.Services.WebServerMode | Network.Services.WebServerMode | Enable web server
clear Network2.Enabled | Network2.Enabled | Flag to determine whether to enable secondary VLAN
clear Network2.Vlan.ManualVlanId | Network2.Vlan.ManualVlanId | User configured VLAN ID of secondary VLAN
clear Network2.Proxy.AutoDiscover | Network2.Proxy.AutoDiscover | Enable WPAD - Web Proxy Auto-Discovery Protocol
clear Network2.Proxy.PacUrl | Network2.Proxy.PacUrl | PAC Configuration URL
clear Network2.Proxy.UserName | Network2.Proxy.UserName | Proxy server login name
clear Network2.Proxy.Password | Network2.Proxy.Password | Proxy server login password
clear Provisioning.CfgChange.UserAcknowledgementEnabled | Provisioning.CfgChange.UserAcknowledgementEnabled | Flag to determine if user acknowledgement is enabled when a configuration change triggers reboot or software update.
clear Provisioning.Server.Static | Provisioning.Server.Static | Flag to determine whether to enable static configuration of the provisioning server address. If true, the provisioning server is configurable through Provisioning.Server.Address. If false, the provisioning server information is discovered using bluetooth, DHCP or DNS SRV record.
clear Provisioning.Server.PrivacyBlock | Provisioning.Server.PrivacyBlock | Flag to disable all uploads that can violate customer privacy.
clear Provisioning.Server.DiscoveryMethod | Provisioning.Server.DiscoveryMethod | Provisioning discovery method
clear Provisioning.Server.Type | Provisioning.Server.Type | Provisioning server type
clear Provisioning.Server.Address | Provisioning.Server.Address | Provisioning server address. Note: Enabled only when Provisioning.Server.Static is set to true.
clear Provisioning.Server.Username | Provisioning.Server.Username | Provisioning server login name. For example, for Provisioning.Server.Type=ftp, this is the user name for logging into the FTP server.
clear Provisioning.Server.Password | Provisioning.Server.Password | Provisioning server login password. For example, for Provisioning.Server.Type=ftp, this is the password for logging into the FTP server.
clear Provisioning.Server.UploadDir | Provisioning.Server.UploadDir | Directory on provisioning server for uploaded files
clear Provisioning.Scheduled.Enable | Provisioning.Scheduled.Enable | Flag to determine if scheduled provisioning is enabled
clear Provisioning.Scheduled.StartTime | Provisioning.Scheduled.StartTime | Scheduled reprovisioning start time
clear Provisioning.Scheduled.Duration | Provisioning.Scheduled.Duration | Scheduled reprovisioning interval duration, reprovisioning will happen randomly within this time frame from the start time
clear Provisioning.InvalidCertificates.AcceptedDigests | Provisioning.InvalidCertificates.AcceptedDigests |
clear Sip.Account.DisplayName | Sip.Account.DisplayName | SIP user display name
clear Sip.Account.UserName | Sip.Account.UserName | Extension Number/Address (also used as SIP user name)
clear Sip.Account.DisplayNumber | Sip.Account.DisplayNumber | This is the number that will be displayed on the home screen, if not configured then extension number will be displayed instead.
clear Sip.Account.TransportType | Sip.Account.TransportType | Preferred transport to communicate with the IP PBX Server
clear Sip.Account.SecureMedia | Sip.Account.SecureMedia | Option to specify if secure media (SRTP/SRTCP) is mandatory or optional, applicable only when TLS transport is active
clear Sip.Account.SelfPort | Sip.Account.SelfPort | Bind port used for SIP transport. TLS port will be default to UDP/TCP port + 1
clear Sip.Pbx.Domain | Sip.Pbx.Domain | The SIP domain is the domain name of the IP PBX service the device is registering with. It should be configured if the device connects to the IP PBX service through one or more SIP Proxies. Leave blank if the device directly connects to the SIP server without going through a SIP proxy.
clear Sip.Pbx.OutboundProxy1 | Sip.Pbx.OutboundProxy1 | Primary call server or outbound proxy address
clear Sip.Pbx.OutboundProxy1Port | Sip.Pbx.OutboundProxy1Port | Primary call server/Outbound proxy port
clear Sip.Pbx.OutboundProxy2 | Sip.Pbx.OutboundProxy2 | Secondary call server or outbound proxy address
clear Sip.Pbx.OutboundProxy2Port | Sip.Pbx.OutboundProxy2Port | Secondary SIP server/Outbound Proxy port
clear Sip.Pbx.SipUriScheme | Sip.Pbx.SipUriScheme | SIP URI Scheme. When set to true it's sip, when it's set to false it's sips (Secure SIP)
clear Sip.Pbx.OnlyAcceptCallServerEvents | Sip.Pbx.OnlyAcceptCallServerEvents | Defines whether the device will only accept SIP events from the IP PBX server
clear Sip.Pbx.RegistrationTimeout | Sip.Pbx.RegistrationTimeout | SIP server registration timeout (seconds)
clear Sip.Pbx.Codecs | Sip.Pbx.Codecs | PBX Codec list
clear Sip.Pbx.InBandDTMF | Sip.Pbx.InBandDTMF | In-band DTMF
clear Sip.Credential.Name | Sip.Credential.Name | User credential name
clear Sip.Credential.Password | Sip.Credential.Password | User credential password
clear Sip.Credential.Realm | Sip.Credential.Realm | Server realm
clear Sip.NAT.KeepAliveTimeout | Sip.NAT.KeepAliveTimeout | The keep-alive interval in seconds. Sets the interval at which phones will send a keep-alive packet to the gateway/NAT device to keep the communication port open so that NAT can continue to function.
clear Sip.Vad.SignalAnnexB | Sip.Vad.SignalAnnexB | Flag to specify if G729 Annex B should be signaled.
clear Dvms.InactiveTalkerTimeout | Dvms.InactiveTalkerTimeout | In BT MeetMe, this parameter defines the timeout to decide when a recent talker becomes inactive so he or she can be removed from the active speaker view
clear Dvms.HostPasscode | Dvms.HostPasscode | Chairperson passcode to quickly start meetings. Only applicable when personal mode is enabled.
clear Dvms.Service.Provider | Dvms.Service.Provider | Select a service provider from the list
clear Dvms.Service.Type | Dvms.Service.Type | Select the conferencing service provider application type
clear Dvms.Service.Logo | Dvms.Service.Logo | Select the Dolby Voice audio conferencing service provider logo, that will be displayed on the home screen of the device.
clear Dvms.Service.Name | Dvms.Service.Name | Set the Dolby Voice conferencing service name that will appear on the home screen of the device.
clear Dvms.Service.EnableBluetoothAdvertisement | Dvms.Service.EnableBluetoothAdvertisement | Allow/disallow Bluetooth Advertisement on DCP
clear Dvms.Location.CountryCode | Dvms.Location.CountryCode | Default country code for dial-out
clear Dvms.Server.SIPRegistrationRequired | Dvms.Server.SIPRegistrationRequired | Flag to determine if SIP registration is required with the Dolby Voice Conferencing Server
clear Dvms.Server.Address | Dvms.Server.Address | Dolby Voice server IP address or domain
clear Dvms.Server.Codec | Dvms.Server.Codec | Defines the codec in the SIP SDP offer when connecting to Dolby Voice Conferencing Service
clear Dvms.Server.RegistrationPIN | Dvms.Server.RegistrationPIN | Dolby Voice Registration PIN
clear Dvms.Server.LogALine | Dvms.Server.LogALine | Enable/Disable conference service logging
clear Dvms.PeerDevice.BluetoothId | Dvms.PeerDevice.BluetoothId | Peer device bluetooth ID
clear Dvms.PeerDevice.IpAddress | Dvms.PeerDevice.IpAddress | Peer device IP Address
clear Dvms.Proxy.Address | Dvms.Proxy.Address | Dolby Voice Conference Proxy Address
clear Dvms.Proxy.Port | Dvms.Proxy.Port | Dolby Voice Conference Proxy Port
clear Dvms.Proxy.User | Dvms.Proxy.User | Dolby Voice Conference Proxy User
clear Dvms.Proxy.Password | Dvms.Proxy.Password | Dolby Voice Conference Proxy Password
clear Dvms.Custom.Parameter1 | Dvms.Custom.Parameter1 | Parameter 1 to store the custom configuration
clear Dvms.Custom.Parameter2 | Dvms.Custom.Parameter2 | Parameter 2 to store the custom configuration
clear Dvms.Custom.Parameter3 | Dvms.Custom.Parameter3 | Parameter 3 to store the custom configuration
clear Dvms.Custom.Parameter4 | Dvms.Custom.Parameter4 | Parameter 4 to store the custom configuration
clear Dvms.Custom.SecureParameter1 | Dvms.Custom.SecureParameter1 | Secure parameter 1 to store the custom configuration
clear Dvms.Custom.SecureParameter2 | Dvms.Custom.SecureParameter2 | Secure parameter 2 to store the custom configuration
clear Dvms.Custom.SecureParameter3 | Dvms.Custom.SecureParameter3 | Secure parameter 3 to store the custom configuration
clear Dvms.Custom.SecureParameter4 | Dvms.Custom.SecureParameter4 | Secure parameter 4 to store the custom configuration
clear Dvms.DeveloperMode.Enabled | Dvms.DeveloperMode.Enabled | Turn on developer mode for the Dolby Conference Phone Conferencing App
clear Dvms.Audio.SpatialCaptureOrigin | Dvms.Audio.SpatialCaptureOrigin | To help with audio/video congruence, this parameter allows the application to specify the spatial capture origin so that the audio and video can be aligned
clear Dvms.Audio.RoomSize | Dvms.Audio.RoomSize | Optimize performance for a room of this size
clear Directory.Ldap.URIList | Directory.Ldap.URIList | Comma-separated list of LDAP server URIs (ldap://xxx[,ldap://yyy])
clear Directory.Ldap.LoginName | Directory.Ldap.LoginName | Name used to login into the LDAP server(s)
clear Directory.Ldap.Password | Directory.Ldap.Password | Password used to login into the LDAP server(s)
clear Directory.Ldap.SecureConnection | Directory.Ldap.SecureConnection | Flag to determine whether to use a secure connection to the LDAP server
clear Directory.Ldap.BaseDN | Directory.Ldap.BaseDN | Base domain name for the search. For example, "dc=dolby,dc=com"
clear Directory.Ldap.SearchFilter | Directory.Ldap.SearchFilter | LDAP search filter, where %1 is a placeholder for the search keyword
clear Directory.Ldap.SearchScope | Directory.Ldap.SearchScope | Search depth, where 0=base, 1=one level down, and 2=sub-tree
clear Directory.Ldap.SearchTimeout | Directory.Ldap.SearchTimeout | Search timeout (seconds)
clear Directory.Ldap.SearchLimit | Directory.Ldap.SearchLimit | Maximum number of search results
clear Directory.Ldap.AttrFirstName | Directory.Ldap.AttrFirstName | Name of the attribute corresponding to the first name in the LDAP schema
clear Directory.Ldap.AttrLastName | Directory.Ldap.AttrLastName | Name of the attribute corresponding to the last name in the LDAP schema
clear Directory.Ldap.AttrNumber | Directory.Ldap.AttrNumber | Name of the attribute corresponding to the phone number in the LDAP schema
clear Directory.Ldap.AttrUUID | Directory.Ldap.AttrUUID | Name of the attribute corresponding to the unique user ID in the LDAP schema
clear Directory.Ldap.AttrMail | Directory.Ldap.AttrMail | Name of the attribute corresponding to the e-mail address in the LDAP schema
clear Logging.Upload.Enable | Logging.Upload.Enable | Flag to determine if upload of log files is enabled
clear Logging.Upload.Interval | Logging.Upload.Interval | Interval between logs uploads in minutes
clear Logging.RemoteSyslog.Enable | Logging.RemoteSyslog.Enable | Turn on or off syslog client on the Dolby Conference Phone, configure syslog server IP address to complete the setup
clear Logging.RemoteSyslog.Address | Logging.RemoteSyslog.Address | Syslog server IP address
clear Logging.Console.EnableOutput | Logging.Console.EnableOutput | Flag to determine if sending of logging messages to active console(s) is enabled
clear Logging.Level.Evs | Logging.Level.Evs | EVS (Event Service) is an internal communication dispatch service that allows software modules to talk to each other. In the log file, the module name is EVS.
clear Logging.Level.ACME | Logging.Level.ACME | ACME SDK is a 3rd party library that handles tunneling connection with the conferencing service. In the log file, the module name is ACME.
clear Logging.Level.DVTSC | Logging.Level.DVTSC | DVTSC SDK is a Dolby library that handles tunneling connection with the conferencing service. In the log file, the module name is DVTS.
clear Logging.Level.Sip | Logging.Level.Sip | SIP Communication module, which handles all telephony and conferencing service session negotiation signaling. In the log file, the module name is SIP.
clear Logging.Level.Ccapi | Logging.Level.Ccapi | Conference Control API which handles conferencing service signaling for BT MeetMe, such as roster list, active speaker, device registration, etc. In the log file, the module name is CCAPI.
clear Logging.Level.Api | Logging.Level.Api | APS API is an application programming interface that is used by the Embedded UI and Web UI. In the log file, the module name is API.
clear Logging.Level.Cfg | Logging.Level.Cfg | Configuration manager which handles the storage, dispatch of the configuration parameters. In the log file, the module name is CFG.
clear Logging.Level.Auth | Logging.Level.Auth | Authentication module handles user login from the Web UI as well as the SSH shell. In the log file, the module name is AUTH.
clear Logging.Level.Web | Logging.Level.Web | Web FastCGI module handles the device Web UI requests for device control and diagnostics. In the log file, the module name is WEB.
clear Logging.Level.Ldp | Logging.Level.Ldp | LDAP (Lightweight Directory Access Protocol) handles the LDAP server search request. In the log file, the module name is LDP.
clear Logging.Level.Net | Logging.Level.Net | Network service module handles network configuration such as VLAN, DHCP, LLDP, etc. In the log file the module name is NET.
clear Logging.Level.Pvs | Logging.Level.Pvs | Provisioning service module handles device interactions with the Provisioning Server. The Provisioning Server is a centralized file server that helps to bulk configure the devices and collect logs. In the log file, the module name is PVS.
clear Logging.Level.Shl | Logging.Level.Shl | Shell service handles the SSH shell. In the log file, the module name is SHL.
clear Logging.Level.Upd | Logging.Level.Upd | Update service handles the software upgrade process on the device. In the log file, the module name is UPD.
clear Logging.Level.Dev | Logging.Level.Dev | Device Manager handles the device hardware-related tasks. In the log file, the module name is DEV.
clear Logging.Level.CallLog | Logging.Level.CallLog | Call Log handles the recent call service, records the calls placed, received and missed on the device. In the log file, the module name is CDR.
clear Logging.Level.UI | Logging.Level.UI | Embedded UI User interface module. In the log file, the module name is UI.
clear Logging.Level.Security | Logging.Level.Security | Security module handles the certificate management of the device. In the log file, the module name is SEC.
clear Logging.Level.Cdsp | Logging.Level.Cdsp | DSP (Digital Signal Processor) handles audio processing. In the log file, the module name is CDSP.
clear Logging.Level.BLE | Logging.Level.BLE | Bluetooth module. In the log file, the module name is BLE.
clear Logging.Level.DCC | Logging.Level.DCC | DCC (Dolby Conferencing Console) module is responsible for communications with the DCC server. In the log file, the module name is DCC.
clear Logging.Audio.Mode | Logging.Audio.Mode | Audio module logging level. Possible options are Disabled, Statistics, Diagnostic)
clear Logging.Audio.BufferSize | Logging.Audio.BufferSize | Audio logging buffer size in kB. Possible values range from 4096 to 16384
clear Logging.Audio.EchoRefInputEnabled | Logging.Audio.EchoRefInputEnabled | Flag to determine if logging of echo reference input is enabled
clear Logging.Audio.EchoRefOutputEnabled | Logging.Audio.EchoRefOutputEnabled | Flag to determine if logging of echo reference output is enabled
clear Logging.Audio.JitterInputEnabled | Logging.Audio.JitterInputEnabled | Flag to determine if logging of jitter buffer input is enabled
clear Logging.Audio.JitterOutputEnabled | Logging.Audio.JitterOutputEnabled | Flag to determine if logging of jitter buffer output is enabled
clear Logging.ReportFreeMemory | Logging.ReportFreeMemory | Add memory usage report to each logging entry of the services application
clear Device.SetupCompleted | Device.SetupCompleted | Shows device setup completion status
clear Device.Status.Reboot | Device.Status.Reboot | Shows device reboot status
clear Device.App.Status | Device.App.Status | Application status
clear Device.App.Version | Device.App.Version | Application version
clear Device.App.Name | Device.App.Name | Application name
clear Device.OOBApp.Address | Device.OOBApp.Address | OOBE Application URL
clear Device.AppRecording | Device.AppRecording | Enables the recording of mouse actions from the Applicatiion
clear Device.ReportCrashToDolby | Device.ReportCrashToDolby | Enables the reporting of diagnostics information to Dolby error reporting service
clear Authentication.Local.Admin | Authentication.Local.Admin | Administrative password
clear Authentication.Local.SessionTimeout | Authentication.Local.SessionTimeout | Default authenticated session timeout in seconds. A session is created when a user logs in from Web UI or command line interface
clear Authentication.Local.SessionPurgeTime | Authentication.Local.SessionPurgeTime | The expired sessions record will be purged from the internal sessions list after this many seconds
clear Authentication.Local.AccessPin | Authentication.Local.AccessPin | Phone access PIN. Only applicable when secured access is enabled.
clear Authentication.Local.AutoLockDuration | Authentication.Local.AutoLockDuration | Duration of auto-lock timeout. Only applicable when secured access is enabled for personal mode in the BT MeetMe scenario.