### 1.0Configuration Parameters

The configuration parameters are listed in this section in alphabetical order.

- Features
- Preferences
- Network
- Network2
- Provisioning
- Sip
- Dvms
- Directory
- Logging
- Authentication

Note: Changes to the parameters ending with '*' will cause a phone reboot.

#### 1.1Features

These parameters define the features on the Dolby Conference Phone.

Table 1-1Features Parameters

Parameter | Description | Permitted Values | Default | Provisionable | Web UI Location
--- | --- | --- | --- | --- | ---
Features.OperationMode* | Device operational mode | DUALMODE IPPBXONLYMODE CONFONLYMODE | IPPBXONLYMODE | Yes | Settings / Features / Operation Mode
Features.RecentCallsEnabled | Flag to determine whether to enable the recent calls feature | true, false | true | Yes | Settings / Features / Enable Recent Calls
Features.UserFeedback.Enabled | Flag to determine whether to show the call quality feedback dialog at the end of a call | true, false | true | Yes | Settings / Features / User Feedback / Enable the Call Quality Feedback dialog
Features.UserFeedback.Hotline | User feedback hotline number | 15-character string |  | Yes | Settings / Features / User Feedback / User Feedback Hotline
Features.PersonalMode.Enabled | By enabling this feature, the phone's owner can save his or her chairperson or host passcode to easily start meetings | true, false | false | Yes | Settings / Features / Personal Mode / Set phone for personal use
Features.PersonalMode.SecuredAccessEnabled | Personal PIN authentication required. Only applicable when personal mode is enabled. | true, false | true | Yes | Settings / Features / Personal Mode / Personal PIN authenticate required

#### 1.2Preferences

These parameters define the user preferences on the Dolby Conference Phone.

Table 1-2Preferences Parameters

Parameter | Description | Permitted Values | Default | Provisionable | Web UI Location
--- | --- | --- | --- | --- | ---
Preferences.DndEnabled | Flag to determine whether to enable the Do Not Disturb feature | true, false | false | Yes | Settings / User Preferences / Do Not Disturb
Preferences.AutoAnswerEnabled | Flag to determine whether to enable the Auto-Answer feature | true, false | false | Yes | Settings / User Preferences / Auto-Answer
Preferences.ForwardAllNumber | Phone number to which all calls are forwarded | 15-character string |  | Yes | Settings / User Preferences / Call Forward All Number
Preferences.ForwardBusyNumber | Phone number to which a call is forwarded when the user is busy | 15-character string |  | Yes | Settings / User Preferences / Call Forward Busy Number
Preferences.ForwardNoAnswerNumber | Phone number to which a call is forwarded when the user does not answer the call | 15-character string |  | Yes | Settings / User Preferences / Call Forward No Answer Number
Preferences.SpeechVolume | Speech volume when the Dolby Conference Phone is on a call | 1 to 20 | 14 | Yes | Settings / User Preferences / Speech Volume
Preferences.RingerVolume | Ringer volume | 1 to 20 | 10 | Yes | Settings / User Preferences / Ringer Volume
Preferences.BrightnessLevel | Brightness level of backlight | 0 to 100 | 80 | Yes | Settings / User Preferences / Brightness Level
Preferences.SystemNotificationSounds | Turn on or off the system notification sounds | true, false | true | Yes | Settings / User Preferences / System Notification Sounds
Preferences.ShowSystemWarning | Show system warning on the phone | true, false | true | Yes | Settings / User Preferences / Show System Warning
Preferences.Localization.Timezone | Time zone where the device is located | Pacific/Kwajalein Pacific/Samoa Pacific/Honolulu America/Anchorage America/Los_Angeles America/Denver America/Chicago America/New_York America/Caracas America/St_Johns America/Argentina/Buenos_Aires Atlantic/South_Georgia Atlantic/Azores Europe/London Europe/Paris Africa/Johannesburg Asia/Baghdad Asia/Tehran Asia/Muscat Asia/Kabul Asia/Karachi Asia/Kolkata Asia/Kathmandu Asia/Dhaka Asia/Bangkok Asia/Singapore Asia/Tokyo Australia/Adelaide Australia/Sydney Asia/Magadan Pacific/Auckland | Europe/London | Yes | Settings / User Preferences / Localization / Time Zone
Preferences.Localization.TimeFormat | Time Format | h:mm ap h:mm | h:mm ap | Yes | Settings / User Preferences / Localization / Time Format
Preferences.Localization.DateFormat | Date Format | dd/MM/yy d MMMM, yyyy MMMM d, yyyy MM/dd/yy d MMM, yy MMM d, yy d MMMM yyyy dd.MM.yy d. MMMM yyyy Spanish/Portuguese long Chinese long yyyy/MM/dd yy. M. d. Korean long dd/MM/yyyy | MMMM d, yyyy | No | Settings / User Preferences / Localization / Date Format
Preferences.Localization.Language | Language preference for the embedded UI | en fr it de es pt pt_BR zh-Hant zh-Hans ja ko ar he | en | Yes | Settings / User Preferences / Localization / Language

#### 1.3Network

These parameters specify the network connections for the Dolby Conference Phone.

Table 1-3Network Parameters

Parameter | Description | Permitted Values | Default | Provisionable | Web UI Location
--- | --- | --- | --- | --- | ---
Network.DHCP* | Flag to determine whether to enable automatic network configuration using DHCP. If true, the phone will request an IP address from the DHCP server. If set to false, the user must manually configure the IP address | true, false | true | No | Settings / Network / DHCP Network Configuration Method
Network.IpAddress* | IP address of the phone. Note: Enabled only when Network.DHCP is set to false. | 15-character string |  | No | Settings / Network / IP Address
Network.Subnet* | Subnet mask of the network interface. Note: Enabled only when Network.DHCP is set to false. | 15-character string |  | No | Settings / Network / Subnet Mask
Network.DefaultGateway | Default gateway for IP Routing. Note: Enabled only when Network.DHCP is set to false. | 15-character string |  | No | Settings / Network / Default Gateway
Network.ManualDNS | Override DHCP assigned DNS settings | true, false | false | No | Settings / Network / Override DHCP assigned DNS Settings
Network.DomainName | Network domain name | DOMAIN |  | No | Settings / Network / Domain Name
Network.DNS1 | Primary DNS server IP address. Note: Enabled only when Network.DHCP is set to false. | 15-character string |  | No | Settings / Network / DNS Server Address
Network.DNS2 | Secondary DNS server IP address. Note: Enabled only when Network.DHCP is set to false. | 15-character string |  | No | Settings / Network / Alternative DNS Server Address
Network.Eapol.Identity* | IEEE 802.1X user identity | 64-character string |  | No | Settings / Network / IEEE 802.1X / IEEE 802.1X User Identity
Network.Eapol.Password* | IEEE 802.1X password | 64-character string |  | No | Settings / Network / IEEE 802.1X / IEEE 802.1X Password
Network.Ntp.Server1 | Primary NTP server IP address | DOMAIN | time.nist.gov | Yes | Settings / Network / NTP / Primary NTP Server Address
Network.Ntp.Server2 | Secondary NTP server IP address | DOMAIN | pool.ntp.org | Yes | Settings / Network / NTP / Secondary NTP Server Address
Network.Vlan.ManualVlanId* | User configured VLAN ID. When DHCP does not provide the VLAN ID, this value is used. | 0 to 4095 | 0 | No | Settings / Network / Virtual LAN / Manual VLAN ID
Network.QoS.DscpVoice | Network layer DSCP priority of voice channels | 0 to 63 | 46 | Yes | Settings / Network / Quality Of Service / DSCP Priority of Voice Channels
Network.QoS.DscpSignaling | Network layer DSCP priority of signaling channels | 0 to 63 | 40 | Yes | Settings / Network / Quality Of Service / DSCP Priority of Signaling Channels
Network.QoS.CosVoice | Link layer priority of voice channels | 0 to 7 | 5 | Yes | Settings / Network / Quality Of Service / Link Layer Priority of Voice Channels
Network.QoS.CosSignaling | Link layer priority of signaling channels | 0 to 7 | 3 | Yes | Settings / Network / Quality Of Service / Link Layer Priority of Signaling Channels
Network.Proxy.AutoDiscover | Enable WPAD - Web Proxy Auto-Discovery Protocol | true, false | false | Yes | Settings / Network / Proxy / Enable WPAD
Network.Proxy.PacUrl | PAC (Proxy Auto Configuration) file URL | ASCII |  | Yes | Settings / Network / Proxy / PAC Configuration URL
Network.Proxy.UserName | Proxy server login name | 64-character string |  | Yes | Settings / Network / Proxy / Proxy Server Login Name
Network.Proxy.Password | Proxy server login password | 64-character string |  | Yes | Settings / Network / Proxy / Proxy Server Login Password
Network.Proxy.EnableCache* | Enable PAC Cache | true, false | true | Yes | Settings / Network / Proxy / Enable PAC Cache
Network.Services.LLDPEnabled* | Enable LLDP | true, false | true | No | Settings / Network / Services / Enable LLDP
Network.Services.SSHEnabled | Enable SSH server | true, false | true | Yes | Settings / Network / Services / Enable SSH Server
Network.Services.WebServerMode | Enable web server | DISABLED ENABLED HTTPSONLY | ENABLED | Yes | Settings / Network / Services / Enable Web Server

#### 1.4Network2

These parameters specify the secondary VLAN for the Dolby Conference Phone.

Table 1-4Network2 Parameters

Parameter | Description | Permitted Values | Default | Provisionable | Web UI Location
--- | --- | --- | --- | --- | ---
Network2.Enabled* | Flag to determine whether to enable secondary VLAN | true, false | false | Yes | Settings / Network - Secondary VLAN / Enable Secondary VLAN
Network2.Vlan.ManualVlanId* | User configured VLAN ID of secondary VLAN | 0 to 4095 | 0 | Yes | Settings / Network - Secondary VLAN / Virtual LAN / Manual VLAN ID
Network2.Proxy.AutoDiscover | Enable WPAD - Web Proxy Auto-Discovery Protocol | true, false | false | Yes | Settings / Network - Secondary VLAN / Proxy / Enable WPAD
Network2.Proxy.PacUrl | PAC Configuration URL | ASCII |  | Yes | Settings / Network - Secondary VLAN / Proxy / PAC Configuration URL
Network2.Proxy.UserName | Proxy server login name | 64-character string |  | Yes | Settings / Network - Secondary VLAN / Proxy / Proxy Server Login Name
Network2.Proxy.Password | Proxy server login password | 64-character string |  | Yes | Settings / Network - Secondary VLAN / Proxy / Proxy Server Login Password

#### 1.5Provisioning

These parameters specify the connection to the provisioning server.

Table 1-5Provisioning Parameters

Parameter | Description | Permitted Values | Default | Provisionable | Web UI Location
--- | --- | --- | --- | --- | ---
Provisioning.CfgChange.UserAcknowledgementEnabled | Flag to determine if user acknowledgement is enabled when a configuration change triggers reboot or software update. | true, false | true | Yes | Settings / Provisioning / On Configuration Change / User acknowledgement enabled
Provisioning.Server.Static* | Flag to determine whether to enable static configuration of the provisioning server address. If true, the provisioning server is configurable through Provisioning.Server.Address. If false, the provisioning server information is discovered using bluetooth, DHCP or DNS SRV record. | true, false | false | No | Settings / Provisioning / Server / Manual Server Configuration
Provisioning.Server.PrivacyBlock | Flag to disable all uploads that can violate customer privacy. | true, false | false | No | Settings / Provisioning / Server / Disable Privacy-related Uploads
Provisioning.Server.Type | Provisioning server type | FTP HTTP HTTPS | FTP | No | Settings / Provisioning / Server / Provisioning Server Type
Provisioning.Server.Address | Provisioning server address. Note: Enabled only when Provisioning.Server.Static is set to true. | 256-character string |  | No | Settings / Provisioning / Server / Provisioning Server Address
Provisioning.Server.Username | Provisioning server login name. For example, for Provisioning.Server.Type=ftp, this is the user name for logging into the FTP server. | 64-character string |  | No | Settings / Provisioning / Server / Provisioning Server Login Name
Provisioning.Server.Password | Provisioning server login password. For example, for Provisioning.Server.Type=ftp, this is the password for logging into the FTP server. | 64-character string |  | No | Settings / Provisioning / Server / Provisioning Server Login Password
Provisioning.Server.UploadDir | Directory on provisioning server for uploaded files | 512-character string |  | Yes | Settings / Provisioning / Server / Upload Directory
Provisioning.Scheduled.Enable | Flag to determine if scheduled provisioning is enabled | true, false | false | Yes | Settings / Provisioning / Scheduled Provisioning / Enable scheduled provisioning
Provisioning.Scheduled.StartTime | Scheduled reprovisioning start time | 0 to 23 | 0 | Yes | Settings / Provisioning / Scheduled Provisioning / Scheduled reprovisioning start time (hour)
Provisioning.Scheduled.Duration | Scheduled reprovisioning interval duration, reprovisioning will happen randomly within this time frame from the start time | 5 to 120 | 60 | Yes | Settings / Provisioning / Scheduled Provisioning / Scheduled reprovisioning interval duration (minutes)

#### 1.6Sip

These parameters specify the connection to the call server (or SIP server).

Table 1-6Sip Parameters

Parameter | Description | Permitted Values | Default | Provisionable | Web UI Location
--- | --- | --- | --- | --- | ---
Sip.Account.DisplayName | SIP user display name | 64-character string | Dolby Voice | Yes | Settings / IP PBX Settings / Account / Display Name
Sip.Account.UserName | Extension Number/Address (also used as SIP user name) | 64-character string |  | Yes | Settings / IP PBX Settings / Account / Extension Number/Address
Sip.Account.DisplayNumber | This is the number that will be displayed on the home screen, if not configured then extension number will be displayed instead. | 16-character string |  | Yes | Settings / IP PBX Settings / Account / Display Number
Sip.Account.TransportType | Preferred transport to communicate with the IP PBX Server | AUTO UDP TCP TLS | AUTO | Yes | Settings / IP PBX Settings / Account / Transport Type
Sip.Account.SecureMedia | Option to specify if secure media (SRTP/SRTCP) is mandatory or optional, applicable only when TLS transport is active | MANDATORY OPTIONAL | MANDATORY | Yes | Settings / IP PBX Settings / Account / Secure Media
Sip.Account.SelfPort* | Bind port used for SIP transport. TLS port will be default to UDP/TCP port + 1 | 500 to 9998 | 5060 | Yes | Settings / IP PBX Settings / Account / Transport Port
Sip.Pbx.Domain | The SIP domain is the domain name of the IP PBX service the device is registering with. It should be configured if the device connects to the IP PBX service through one or more SIP Proxies. Leave blank if the device directly connects to the SIP server without going through a SIP proxy. | 64-character string |  | Yes | Settings / IP PBX Settings / Server / SIP Domain Name
Sip.Pbx.OutboundProxy1 | Primary call server or outbound proxy address | DOMAIN |  | Yes | Settings / IP PBX Settings / Server / Primary Call Server/Outbound Proxy
Sip.Pbx.OutboundProxy1Port | Primary call server/Outbound proxy port | 500 to 65534 | 5060 | Yes | Settings / IP PBX Settings / Server / Primary Server/Outbound Proxy Port
Sip.Pbx.OutboundProxy2 | Secondary call server or outbound proxy address | DOMAIN |  | Yes | Settings / IP PBX Settings / Server / Secondary Call Server/Outbound Proxy
Sip.Pbx.OutboundProxy2Port | Secondary SIP server/Outbound Proxy port | 500 to 65534 | 5060 | Yes | Settings / IP PBX Settings / Server / Secondary Server/Outbound Proxy Port
Sip.Pbx.SipUriScheme | SIP URI Scheme. When set to true it's sip, when it's set to false it's sips (Secure SIP) | true, false | true | Yes | Settings / IP PBX Settings / Server / SIP URI Scheme
Sip.Pbx.OnlyAcceptCallServerEvents | Defines whether the device will only accept SIP events from the IP PBX server | true, false | true | Yes | Settings / IP PBX Settings / Server / Only accept call server SIP events
Sip.Pbx.RegistrationTimeout* | SIP server registration timeout (seconds) | 5 to 60 | 32 | Yes | Settings / IP PBX Settings / Server / SIP Registration Timeout (seconds)
Sip.Pbx.Codecs | PBX Codec list | 128-character string | G722,G711U,G711A,iLBC,G729AB | Yes | Settings / IP PBX Settings / Server / PBX Codec List
Sip.Pbx.InBandDTMF | In-band DTMF | true, false | false | Yes | Settings / IP PBX Settings / Server / In band DTMF
Sip.Credential.Name | User credential name | 64-character string |  | Yes | Settings / IP PBX Settings / Credential / User Credential Name
Sip.Credential.Password | User credential password | 64-character string |  | Yes | Settings / IP PBX Settings / Credential / User Credential Password
Sip.Credential.Realm | Server realm | 32-character string | * | Yes | Settings / IP PBX Settings / Credential / Server Realm
Sip.NAT.KeepAliveTimeout | The keep-alive interval in seconds. Sets the interval at which phones will send a keep-alive packet to the gateway/NAT device to keep the communication port open so that NAT can continue to function. | 0 to 3600 | 30 | Yes | Settings / IP PBX Settings / NAT / Keep-alive timeout
Sip.Vad.SignalAnnexB | Flag to specify if G729 Annex B should be signaled. | true, false | true | Yes | Settings / IP PBX Settings / VAD / Signal G729 Annex B

#### 1.7Dvms

These parameters specify the connection to the BT MeetMe with Dolby Voice conferencing service.

Table 1-7Dvms Parameters

Parameter | Description | Permitted Values | Default | Provisionable | Web UI Location
--- | --- | --- | --- | --- | ---
Dvms.InactiveTalkerTimeout | In BT MeetMe, this parameter defines the timeout to decide when a recent talker becomes inactive so he or she can be removed from the active speaker view | 10 to 65534 | 60 | Yes | Settings / Dolby Voice Conferencing Service / Inactive Talker Timeout (seconds)
Dvms.HostPasscode | Chairperson passcode to quickly start meetings. Only applicable when personal mode is enabled. | 16-character string |  | No | Settings / Dolby Voice Conferencing Service / Host passcode
Dvms.Service.Provider* | Select a service provider from the list | BT MeetMe Custom | BT MeetMe | Yes | Settings / Dolby Voice Conferencing Service / Service / Service provider
Dvms.Service.Type* | Select the conferencing service provider application type | BT MeetMe CSAF | BT MeetMe | Yes | Settings / Dolby Voice Conferencing Service / Service / Application type
Dvms.Service.Logo | Select the Dolby Voice audio conferencing service provider logo, that will be displayed on the home screen of the device. | BT Dolby Disabled | BT | Yes | Settings / Dolby Voice Conferencing Service / Service / Logo
Dvms.Service.Name | Set the Dolby Voice conferencing service name that will appear on the home screen of the device. | 32-character string | BT MeetMe | Yes | Settings / Dolby Voice Conferencing Service / Service / Name
Dvms.Service.EnableBluetoothAdvertisement | Allow/disallow Bluetooth Advertisement on DCP | true, false | true | Yes | Settings / Dolby Voice Conferencing Service / Service / Allow bluetooth advertisement
Dvms.Location.CountryCode | Default country code for dial-out | 4-character string | 1 | Yes | Settings / Dolby Voice Conferencing Service / Location / Country code
Dvms.Server.SIPRegistrationRequired | Flag to determine if SIP registration is required with the Dolby Voice Conferencing Server | true, false | false | Yes | Settings / Dolby Voice Conferencing Service / Server / SIP Registration Required
Dvms.Server.Address | Dolby Voice server IP address or domain | URL | https://my.webjoin.com/dolby/ws/rest/callcontrol | Yes | Settings / Dolby Voice Conferencing Service / Server / Dolby Voice Conferencing Server Address
Dvms.Server.Codec | Defines the codec in the SIP SDP offer when connecting to Dolby Voice Conferencing Service | 32-character string | 9;G722;8000 | Yes | Settings / Dolby Voice Conferencing Service / Server / Codec
Dvms.Server.RegistrationPIN | Dolby Voice Registration PIN | ASCII | Pin1234567 | Yes | Settings / Dolby Voice Conferencing Service / Server / Dolby Voice Conferencing Server Registration PIN
Dvms.Server.LogALine | Enable/Disable conference service logging | true, false | true | Yes | Settings / Dolby Voice Conferencing Service / Server / Enable Service Logging
Dvms.PeerDevice.IpAddress | Peer device IP Address | 15-character string |  | No | Settings / Dolby Voice Conferencing Service / Peer Device / IP Address
Dvms.Proxy.Address | Dolby Voice Conference Proxy Address | URL |  | Yes | Settings / Dolby Voice Conferencing Service / Proxy / Proxy Address
Dvms.Proxy.Port | Dolby Voice Conference Proxy Port | 1 to 65534 | 8080 | Yes | Settings / Dolby Voice Conferencing Service / Proxy / Proxy Port
Dvms.Proxy.User | Dolby Voice Conference Proxy User | 32-character string |  | Yes | Settings / Dolby Voice Conferencing Service / Proxy / Proxy User
Dvms.Proxy.Password | Dolby Voice Conference Proxy Password | 16-character string |  | Yes | Settings / Dolby Voice Conferencing Service / Proxy / Proxy Password
Dvms.Custom.Parameter1 | Parameter 1 to store the custom configuration | 65536-character string |  | Yes | Settings / Dolby Voice Conferencing Service / Custom / Custom Parameter 1
Dvms.Custom.Parameter2 | Parameter 2 to store the custom configuration | 65536-character string |  | Yes | Settings / Dolby Voice Conferencing Service / Custom / Custom Parameter 2
Dvms.Custom.Parameter3 | Parameter 3 to store the custom configuration | 65536-character string |  | Yes | Settings / Dolby Voice Conferencing Service / Custom / Custom Parameter 3
Dvms.Custom.Parameter4 | Parameter 4 to store the custom configuration | 65536-character string |  | Yes | Settings / Dolby Voice Conferencing Service / Custom / Custom Parameter 4
Dvms.Custom.SecureParameter1 | Secure parameter 1 to store the custom configuration | 2048-character string |  | Yes | Settings / Dolby Voice Conferencing Service / Custom / Secure Custom Parameter 1
Dvms.Custom.SecureParameter2 | Secure parameter 2 to store the custom configuration | 2048-character string |  | Yes | Settings / Dolby Voice Conferencing Service / Custom / Secure Custom Parameter 2
Dvms.Custom.SecureParameter3 | Secure parameter 3 to store the custom configuration | 2048-character string |  | Yes | Settings / Dolby Voice Conferencing Service / Custom / Secure Custom Parameter 3
Dvms.Custom.SecureParameter4 | Secure parameter 4 to store the custom configuration | 2048-character string |  | Yes | Settings / Dolby Voice Conferencing Service / Custom / Secure Custom Parameter 4
Dvms.DeveloperMode.Enabled | Turn on developer mode for the Dolby Conference Phone Conferencing App | true, false | false | Yes | Settings / Dolby Voice Conferencing Service / Developer Mode / Enable developer mode
Dvms.Audio.SpatialCaptureOrigin | To help with audio/video congruence, this parameter allows the application to specify the spatial capture origin so that the audio and video can be aligned | 0 90 180 270 | 0 | Yes | Settings / Dolby Voice Conferencing Service / Audio / Spatial capture origin
Dvms.Audio.RoomSize | Optimize performance for a room of this size | DEFAULT SMALL | DEFAULT | Yes | Settings / Dolby Voice Conferencing Service / Audio / Room size

#### 1.8Directory

These parameters define the directories that are stored on the phone. This includes the LDAP definitions. The LDAP parameters specifies the location of the corporate directory\'s LDAP server, the LDAP attributes, and other settings.

Table 1-8Directory Parameters

Parameter | Description | Permitted Values | Default | Provisionable | Web UI Location
--- | --- | --- | --- | --- | ---
Directory.Ldap.URIList | Comma-separated list of LDAP server URIs (ldap://xxx[,ldap://yyy]) | 128-character string |  | Yes | Settings / Corporate Directory / LDAP / Server URI(s)
Directory.Ldap.LoginName | Name used to login into the LDAP server(s) | 256-character string |  | Yes | Settings / Corporate Directory / LDAP / User Name
Directory.Ldap.Password | Password used to login into the LDAP server(s) | 32-character string |  | Yes | Settings / Corporate Directory / LDAP / Password
Directory.Ldap.SecureConnection | Flag to determine whether to use a secure connection to the LDAP server | true, false | true | Yes | Settings / Corporate Directory / LDAP / Secure Connection
Directory.Ldap.BaseDN | Base domain name for the search. For example, "dc=dolby,dc=com" | 64-character string |  | Yes | Settings / Corporate Directory / LDAP / Base DN
Directory.Ldap.SearchFilter | LDAP search filter, where %1 is a placeholder for the search keyword | 256-character string | (&(objectCategory=person)(|(sn=%1*)(givenName=%1*))(!(msExchHideFromAddressLists=TRUE))) | Yes | Settings / Corporate Directory / LDAP / Search Filter
Directory.Ldap.SearchScope | Search depth, where 0=base, 1=one level down, and 2=sub-tree | 0 to 2 | 2 | Yes | Settings / Corporate Directory / LDAP / Search Depth
Directory.Ldap.SearchTimeout | Search timeout (seconds) | 0 to 60 | 15 | Yes | Settings / Corporate Directory / LDAP / Search Timeout (seconds)
Directory.Ldap.SearchLimit | Maximum number of search results | 0 to 1000 | 200 | Yes | Settings / Corporate Directory / LDAP / Maximum Search Results
Directory.Ldap.AttrFirstName | Name of the attribute corresponding to the first name in the LDAP schema | 32-character string | givenName | Yes | Settings / Corporate Directory / LDAP / First Name Attribute Name
Directory.Ldap.AttrLastName | Name of the attribute corresponding to the last name in the LDAP schema | 32-character string | sn | Yes | Settings / Corporate Directory / LDAP / Last Name Attribute Name
Directory.Ldap.AttrNumber | Name of the attribute corresponding to the phone number in the LDAP schema | 32-character string | telephoneNumber | Yes | Settings / Corporate Directory / LDAP / Phone Number Attribute Name
Directory.Ldap.AttrUUID | Name of the attribute corresponding to the unique user ID in the LDAP schema | 32-character string | uidNumber | Yes | Settings / Corporate Directory / LDAP / UUID Attribute Name
Directory.Ldap.AttrMail | Name of the attribute corresponding to the e-mail address in the LDAP schema | 32-character string | mail | Yes | Settings / Corporate Directory / LDAP / E-Mail Attribute Name

#### 1.9Logging

These parameters specify what information is logged and where it is logged. The level parameters specify the logging levels written to the log file. The remote syslog parameters specify the connection to syslog.

Table 1-9Logging Parameters

Parameter | Description | Permitted Values | Default | Provisionable | Web UI Location
--- | --- | --- | --- | --- | ---
Logging.Upload.Enable | Flag to determine if upload of log files is enabled | true, false | false | Yes | Settings / Logging / Upload Logs / Enable logs uploading
Logging.Upload.Interval | Interval between logs uploads in minutes | 1 to 1440 | 5 | Yes | Settings / Logging / Upload Logs / Log files upload interval
Logging.RemoteSyslog.Enable | Turn on or off syslog client on the Dolby Conference Phone, configure syslog server IP address to complete the setup | true, false | false | Yes | Settings / Logging / Syslog Service / Enable Syslog
Logging.RemoteSyslog.Address | Syslog server IP address | 15-character string |  | Yes | Settings / Logging / Syslog Service / Syslog Server IP Address
Logging.Console.EnableOutput* | Flag to determine if sending of logging messages to active console(s) is enabled | true, false | false | Yes | Settings / Logging / Console Logging / Enable Console Logging
Logging.Level.Evs | EVS (Event Service) is an internal communication dispatch service that allows software modules to talk to each other. In the log file, the module name is EVS. | NONE EMERGENCY ALERT CRITICAL ERROR WARNING NOTICE INFO DEBUG DEBUG1 | INFO | Yes | Settings / Logging / Log Levels / EVS Module
Logging.Level.ACME | ACME SDK is a 3rd party library that handles tunneling connection with the conferencing service. In the log file, the module name is ACME. | NONE EMERGENCY ALERT CRITICAL ERROR WARNING NOTICE INFO DEBUG DEBUG1 | INFO | Yes | Settings / Logging / Log Levels / ACME SDK Module
Logging.Level.DVTSC | DVTSC SDK is a Dolby library that handles tunneling connection with the conferencing service. In the log file, the module name is DVTS. | NONE EMERGENCY ALERT CRITICAL ERROR WARNING NOTICE INFO DEBUG DEBUG1 | INFO | Yes | Settings / Logging / Log Levels / DVTSC SDK Module
Logging.Level.Sip | SIP Communication module, which handles all telephony and conferencing service session negotiation signaling. In the log file, the module name is SIP. | NONE EMERGENCY ALERT CRITICAL ERROR WARNING NOTICE INFO DEBUG DEBUG1 | INFO | Yes | Settings / Logging / Log Levels / SIP Module
Logging.Level.Ccapi | Conference Control API which handles conferencing service signaling for BT MeetMe, such as roster list, active speaker, device registration, etc. In the log file, the module name is CCAPI. | NONE EMERGENCY ALERT CRITICAL ERROR WARNING NOTICE INFO DEBUG DEBUG1 | INFO | Yes | Settings / Logging / Log Levels / CCAPI Module
Logging.Level.Api | APS API is an application programming interface that is used by the Embedded UI and Web UI. In the log file, the module name is API. | NONE EMERGENCY ALERT CRITICAL ERROR WARNING NOTICE INFO DEBUG DEBUG1 | INFO | Yes | Settings / Logging / Log Levels / API Module
Logging.Level.Cfg | Configuration manager which handles the storage, dispatch of the configuration parameters. In the log file, the module name is CFG. | NONE EMERGENCY ALERT CRITICAL ERROR WARNING NOTICE INFO DEBUG DEBUG1 | INFO | Yes | Settings / Logging / Log Levels / CFG Module
Logging.Level.Auth | Authentication module handles user login from the Web UI as well as the SSH shell. In the log file, the module name is AUTH. | NONE EMERGENCY ALERT CRITICAL ERROR WARNING NOTICE INFO DEBUG DEBUG1 | INFO | Yes | Settings / Logging / Log Levels / AUTH Module
Logging.Level.Web | Web FastCGI module handles the device Web UI requests for device control and diagnostics. In the log file, the module name is WEB. | NONE EMERGENCY ALERT CRITICAL ERROR WARNING NOTICE INFO DEBUG DEBUG1 | INFO | Yes | Settings / Logging / Log Levels / WEB Module
Logging.Level.Ldp | LDAP (Lightweight Directory Access Protocol) handles the LDAP server search request. In the log file, the module name is LDP. | NONE EMERGENCY ALERT CRITICAL ERROR WARNING NOTICE INFO DEBUG DEBUG1 | INFO | Yes | Settings / Logging / Log Levels / LDAP Module
Logging.Level.Net | Network service module handles network configuration such as VLAN, DHCP, LLDP, etc. In the log file the module name is NET. | NONE EMERGENCY ALERT CRITICAL ERROR WARNING NOTICE INFO DEBUG DEBUG1 | INFO | Yes | Settings / Logging / Log Levels / NET Module
Logging.Level.Pvs | Provisioning service module handles device interactions with the Provisioning Server. The Provisioning Server is a centralized file server that helps to bulk configure the devices and collect logs. In the log file, the module name is PVS. | NONE EMERGENCY ALERT CRITICAL ERROR WARNING NOTICE INFO DEBUG DEBUG1 | INFO | Yes | Settings / Logging / Log Levels / Provisioning Module
Logging.Level.Shl | Shell service handles the SSH shell. In the log file, the module name is SHL. | NONE EMERGENCY ALERT CRITICAL ERROR WARNING NOTICE INFO DEBUG DEBUG1 | INFO | Yes | Settings / Logging / Log Levels / Shell Module
Logging.Level.Upd | Update service handles the software upgrade process on the device. In the log file, the module name is UPD. | NONE EMERGENCY ALERT CRITICAL ERROR WARNING NOTICE INFO DEBUG DEBUG1 | INFO | Yes | Settings / Logging / Log Levels / Update Module
Logging.Level.Dev | Device Manager handles the device hardware-related tasks. In the log file, the module name is DEV. | NONE EMERGENCY ALERT CRITICAL ERROR WARNING NOTICE INFO DEBUG DEBUG1 | INFO | Yes | Settings / Logging / Log Levels / Device Manager Module
Logging.Level.CallLog | Call Log handles the recent call service, records the calls placed, received and missed on the device. In the log file, the module name is CDR. | NONE EMERGENCY ALERT CRITICAL ERROR WARNING NOTICE INFO DEBUG DEBUG1 | INFO | Yes | Settings / Logging / Log Levels / CALLLOG Module
Logging.Level.UI | Embedded UI User interface module. In the log file, the module name is UI. | NONE EMERGENCY ALERT CRITICAL ERROR WARNING NOTICE INFO DEBUG DEBUG1 | INFO | Yes | Settings / Logging / Log Levels / UI Module
Logging.Level.Security | Security module handles the certificate management of the device. In the log file, the module name is SEC. | NONE EMERGENCY ALERT CRITICAL ERROR WARNING NOTICE INFO DEBUG DEBUG1 | INFO | Yes | Settings / Logging / Log Levels / Security Module
Logging.Level.Cdsp | DSP (Digital Signal Processor) handles audio processing. In the log file, the module name is CDSP. | NONE EMERGENCY ALERT CRITICAL ERROR WARNING NOTICE INFO DEBUG DEBUG1 | INFO | Yes | Settings / Logging / Log Levels / Cdsp Module
Logging.Level.BLE | Bluetooth module. In the log file, the module name is BLE. | NONE EMERGENCY ALERT CRITICAL ERROR WARNING NOTICE INFO DEBUG DEBUG1 | INFO | Yes | Settings / Logging / Log Levels / Bluetooth Module
Logging.Level.DCC | DCC (Dolby Conferencing Console) module is responsible for communications with the DCC server. In the log file, the module name is DCC. | NONE EMERGENCY ALERT CRITICAL ERROR WARNING NOTICE INFO DEBUG DEBUG1 | INFO | Yes | Settings / Logging / Log Levels / DCC Module
Logging.Audio.Mode | Audio module logging level. Possible options are Disabled, Statistics, Diagnostic) | DISABLED STATISTICS DIAGNOSTIC | DISABLED | Yes | Settings / Logging / Audio / Audio Logging Level
Logging.Audio.BufferSize | Audio logging buffer size in kB. Possible values range from 4096 to 16384 | 4096 to 16384 | 16384 | Yes | Settings / Logging / Audio / Audio Logging Total Buffer Size
Logging.Audio.EchoRefInputEnabled | Flag to determine if logging of echo reference input is enabled | true, false | false | Yes | Settings / Logging / Audio / Echo Reference Input
Logging.Audio.EchoRefOutputEnabled | Flag to determine if logging of echo reference output is enabled | true, false | false | Yes | Settings / Logging / Audio / Echo Reference Output
Logging.Audio.JitterInputEnabled | Flag to determine if logging of jitter buffer input is enabled | true, false | false | Yes | Settings / Logging / Audio / Jitter Buffer Input
Logging.Audio.JitterOutputEnabled | Flag to determine if logging of jitter buffer output is enabled | true, false | false | Yes | Settings / Logging / Audio / Jitter Buffer Output
Logging.ReportFreeMemory | Add memory usage report to each logging entry of the services application | true, false | false | No | Settings / Logging / Report Free Memory

#### 1.10Authentication

This parameter defines the authentication parameters for the phone.

Table 1-11Authentication Parameters

Parameter | Description | Permitted Values | Default | Provisionable | Web UI Location
--- | --- | --- | --- | --- | ---
Authentication.Local.Admin | Administrative password | 9-character string | 1739 | Yes | Settings / Authentication / Local Account / Administrative Password
Authentication.Local.SessionTimeout | Default authenticated session timeout in seconds. A session is created when a user logs in from Web UI or command line interface | 0 to 1200 | 180 | Yes | Settings / Authentication / Local Account / Default Session Timeout (seconds)
Authentication.Local.SessionPurgeTime | The expired sessions record will be purged from the internal sessions list after this many seconds | 0 to 1200 | 600 | Yes | Settings / Authentication / Local Account / Expired Sessions Purged Time (seconds)
Authentication.Local.AccessPin | Phone access PIN. Only applicable when secured access is enabled. | 4-character string |  | No | Settings / Authentication / Local Account / Phone access PIN
Authentication.Local.AutoLockDuration | Duration of auto-lock timeout. Only applicable when secured access is enabled for personal mode in the BT MeetMe scenario. | 5_MINUTES 20_MINUTES 1_HOUR 2_HOURS 4_HOURS 8_HOURS | 1_HOUR | Yes | Settings / Authentication / Local Account / Autolock timeout duration